SMU - SECTION 3D & 5C1 - REAR SPINDLE NUT TORQUE. Geo Metro 1992

For 1990-2009 cars

# SMU - SECTION 3D & 5C1 - REAR SPINDLE NUT TORQUE

---------------------------------------------------------------------- SERVICE MANUAL UPDATE ----------------------------------------------------------------------

#### SUBJECT: SECTIONS 3D AND 5C1 - REAR SPINDLE NUT TORQUE SPECIFICATIONS

#### MODELS: 1992-95 GEO METRO

THE TORQUE SPECIFICATIONS FOR THE REAR SPINDLE NUT HAVE BEEN REVISED. PLEASE USE THE FOLLOWING SPECIFICATIONS WHEN SERVICING REAR SPINDLE NUT.

. 1992 THROUGH 1994 GEO METRO MODELS:

100 N.M (74 LB FT)

. 1995 GEO METRO MODELS:

100 N.M (74 LB FT) ON VEHICLES WITHOUT ANTILOCK BRAKE SYSTEM (ABS).

170 N.M (125 LB FT) ON VEHICLES EQUIPPED WITH OPTIONAL ABS (RPO JM4).

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.