SMU - SECTIONS 4, 6 & 7 - REVISED SEALANT INFORMATION. Geo Metro 1996

For 1990-2009 cars

# SMU - SECTIONS 4, 6 & 7 - REVISED SEALANT INFORMATION

#### SUBJECT: SERVICE MANUAL UPDATE - SECTIONS 4, 6 AND 7 - REVISED SEALANT INFORMATION

#### MODELS: 1996 AND PRIOR GEO VEHICLES

THIS BULLETIN IS BEING ISSUED TO UPDATE THE SERVICE INFORMATION CONTAINED IN SECTIONS 4, 6 AND 7 OF THE 1996 AND PRIOR GEO SERVICE MANUALS.

WHEN SERVICING THE DRIVE AXLES, ENGINES OR TRANSMISSIONS/TRANSAXLES, DO NOT USE RTV SILICONE SEALANT, P/N 1052917, AS OUTLINED IN THE SERVICE MANUAL PROCEDURES. USE GOODWRENCH (R) RTV SILICONE GASKET + SEALANT, P/N 12346240.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.