LOOSE LUMBER NOISE AT REAR OF VEHICLE-INSPECT/REPLACE STRUT. Geo Prizm 1990

For 1990-2009 cars

# LOOSE LUMBER NOISE AT REAR OF VEHICLE-INSPECT/REPLACE STRUT

#### Subject: LOOSE LUMBER NOISE FROM REAR OF VEHICLE

#### Model and Year: 1990 GEO PRIZM

A limited number of 1990 GEO Prizms may exhibit a "Loose Lumber" noise emanating from the rear of the vehicle. This noise may be associated with seepage of fluid from the rear strut assemblies. If such a condition exists on a vehicle, a visual inspection of the rear struts may verify if this is in fact the cause:

- Raise the boot of the strut assembly.

- Check for fluid on the rod.

- If fluid is present on either strut, both strut assemblies must be replaced.

P/N 94849286 Strut Assembly RH

P/N 94849288 Strut Assembly LH

Parts are currently available from GMSPO.

Inspection Labor Operation Number: T1586

Inspection Labor Time: .2 Hours

Trouble Code: 92

Replacement Labor Operation Number: E5757

See applicable Labor Time Guide for labor hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.