FALSE SETTING OF SUPPLEMENTAL RESTRAINT SYSTEM (INFORMATION). Geo Prizm 1993

For 1990-2009 cars

# FALSE SETTING OF SUPPLEMENTAL RESTRAINT SYSTEM (INFORMATION)

#### SUBJECT: FALSE SETTING OF SUPPLEMENTAL RESTRAINT SYSTEM

#### MODEL and YEAR: 1993 GEO PRIZM

False setting of Supplemental Restraint System (SRS) diagnostic trouble code 22 "Air Bag Indicator Circuit Fault".

If the electrical harness connectors which attach to the back of the instrument cluster are removed while the battery is connected, and the ignition switch is cycled to the "ON" or "START" position, a trouble code 22 will be set in the SRS diagnostic trouble code memory.

#### CORRECTION:

---------- This code may be removed from the DTC memory using the procedure found in the 1993 Prizm Service Manual. After reconnecting the electrical harness to the instrument cluster and removing the trouble code from the DTC memory, verify that there are no additional reasons for trouble code 22 to be set in the memory.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.