Vehicle Speed Sensor Replacement. Geo Prizm 1996

For 1990-2009 cars

#### Tools Required

J 36850 Transmission Assembly Lubricant

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative (-) battery cable.
2. Disconnect the vehicle speed sensor (VSS) electrical connector.
3. Remove the 1 retaining bolt (1) and the VSS (2) from the transaxle.
4. Inspect the VSS O-ring for cuts or damage. Replace as necessary.

### Installation Procedure

1. Apply J 36850 to the VSS O-ring.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the Vehicle Speed Sensor (VSS) into the transaxle case. Secure the VSS (2) with the retaining bolt (1).

Tighten
Tighten the VSS speed sensor (VSS) bolt to 6 N·m (53 lb in).

3. Connect the VSS electrical connector.
4. Connect the negative (-) battery cable.