Circuit Opening Relay Replacement. Geo Prizm 1996

For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the center console.
3. Remove the circuit opening relay (1) electrical connector.
4. Remove the one bolt and circuit opening from the I/P bracket.

### Installation Procedure

1. Install the circuit opening relay to I/P bracket; secure with one bolt.

Tighten
Tighten the circuit opening relay bolt to 10 N·m (89 lb in).

2. Install the circuit opening relay electrical connector.
3. Install the center console.
4. Connect the negative battery cable.

Tighten
Tighten the negative battery cable-to-negative battery cable terminal retainer to 15N·m (11 lb ft).