Heated Oxygen Sensor Replacement. Geo Prizm 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the throttle body from the intake manifold. Refer to Throttle Body Replacement.
2. Remove the 2 screws and throttle opener from the throttle body.

### Installation Procedure

1. Install the throttle opener to throttle body.
2. Secure the throttle opener with the 2 screws.
3. Install the throttle body to the intake manifold. Refer to Throttle Body Replacement.