Fuel Pump Replacement. Geo Prizm 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement.
2. Loosen the clamp (2) securing the fuel pump to the fuel sender assembly.
3. Disconnect the fuel pump electrical connector (3).
4. Remove the fuel pump (1) from the fuel sender assembly.
5. Remove the fuel pump strainer (1) from the fuel pump (2).

### Installation Procedure

1. Install the fuel pump strainer (1) to the fuel pump (2).
2. Install the fuel pump (1) to the fuel sender assembly.
3. Tighten the clamp (2) securing the fuel pump feed hose to the fuel sender.
4. Connect the fuel pump electrical connector (3).
5. Install the fuel sender to the fuel tank. Refer to Fuel Sender Assembly Replacement.