KEY BREAKAGE LIFTING HATCH (NEW COPPER/NICKEL ALLOY KEY). Geo Spectrum 1989

For 1990-2009 cars

# KEY BREAKAGE LIFTING HATCH (NEW COPPER/NICKEL ALLOY KEY)

#### Subject: KEY BREAKAGE LIFTING HATCH, IN DOOR OR IGNITION

#### Model and Year: 1989 GEO SPECTRUM 1990 GEO STORM 1989-90 GEO METRO, TRACKER

Some 1989-90 GEO M, R cars and J trucks may experience key breakage usually when lifting the hatch, but sometimes in the door or ignition. A new copper/nickel alloy key has been released with a greater resistance to breaking. This key may be cut with either a follower or punch type cutter. The part numbers for this new key are:

96065464 - GEO

This new key has been in production since November, 1990.

Part is currently available from GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.