FRONT SEAT CHUCKING CONDITION CARPET BETWEEN FLOOR/SEAT. Geo Spectrum 1985

For 1990-2009 cars

# FRONT SEAT CHUCKING CONDITION CARPET BETWEEN FLOOR/SEAT

#### VEHICLES AFFECTED: 1985 Chevrolet 'R' Car

#### CONDITION:

---------- Some 1985 'R' cars with VIN serial numbers prior to 444391 may exhibit a chucking condition of the front seat. This condition can be due to the carpet being trapped between the seat mounting and the floor. This can cause a loss of retaining torque at the seat adjuster attachment nuts (2).

#### CORRECTION:

----------- 1. Remove (or sufficiently loosen) the seat adjuster nuts - see Figure 10-72 Item 1 in Service Manual.

2. Remove carpet from underneath seat adjustment in area of attachment. Cut away excess carpet material.

3. Reinstall attaching nuts and torque to specification per Service Manual.

Use applicable labour operation numbers and labour time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.