SMU - SECTION 4D - ADDITION OF DUST COVER TO DRIVE AXLE ASSY.. Geo Sprint 1994

For 1990-2009 cars

# SMU - SECTION 4D - ADDITION OF DUST COVER TO DRIVE AXLE ASSY.

********************************************************************** SERVICE MANUAL UPDATE **********************************************************************

#### SUBJECT: SECTION 4D - ADDITION OF DUST COVER TO DRIVE AXLE ASSEMBLY

#### MODELS: 1994 GEO METRO

THE PROCEDURES IN THIS BULLETIN SERVE AS ADDITIONS TO THE PROCEDURES WHICH ALREADY EXIST IN SECTION 4D "UNIT REPAIR" FOR THE "DRIVE AXLE ASSEMBLY" IN THE 1994 GEO METRO SERVICE MANUAL (ST370-94).

REMOVE OR DISCONNECT (THE FOLLOWING STEP SHOULD BE PERFORMED BETWEEN STEP 1 AND STEP 2.)

. DRIVE SHAFT DUST COVER FROM DRIVE AXLE ASSEMBLY.

INSTALL OR CONNECT

#### TOOL REQUIRED:

J41130 - DRIVE AXLE DUST COVER INSTALLER

(THIS STEP SHOULD BE PERFORMED AFTER STEP 7 AND THE "INSPECT" PROCEDURE.)

8. DRIVE AXLE DUST COVER TO DRIVE AXLE ASSEMBLY USING J41130 (FIGURE 12).

. PRESS DRIVE AXLE DUST COVER ONTO DRIVE AXLE ASSEMBLY BY THREADING NUT ONTO DRIVE AXLE SHAFT. TIGHTEN UNTIL J41130 IS IN CONTACT WITH THE WHEEL SIDE JOINT (AT THIS POINT, DRIVE AXLE DUST COVER IS SET AT PROPER DEPTH). DAMAGE TO THE TOOL MAY OCCUR IF OVER TIGHTENED.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.