CLUTCH SHUDDER LAUNCH OR REVERSE. Geo Sprint 1985

For 1990-2009 cars

# CLUTCH SHUDDER LAUNCH OR REVERSE

#### VEHICLES AFFECTED: 1985 Sprint and Firefly 'M' cars

Some early 1985 'M' cars with manual transmissions may exhibit an objectionable driveline disturbance due to clutch shudder. The shudder usually occurs during vehicle launch in first or reverse gear and is most noticeable on steep grades.

This shudder condition can be corrected by installing the following applicable replacement parts on vehicles built prior to the designated V.I.N.'s.

Replace if V.I.N. Part Description Part Number Is Prior To" ---------------- ----------- ------------ Front Engine Mount 96054436 718398 (USA) 718350 (Chev. Canada) 700553 (Pont. Canada) Rear Engine Mount 96051607 703133

Drive Axles (Right and Left) 96053768/9 703024

Use applicable Labour Time and Operation Number.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.