UPDATE-CHILD RESTRAINT SEAT TOP TETHER ANCHOR LOCATION. Geo Sprint 1989

For 1990-2009 cars

# UPDATE-CHILD RESTRAINT SEAT TOP TETHER ANCHOR LOCATION

#### Model and Year: 1989 GEO METRO

#### TO: ALL CHEVROLET DEALERS

CHEVROLET DEALER SERVICE BULLETIN 89-121-10 DATED APRIL, 1989 INCORRECTLY REFERENCED TRACKER AS THE MODEL AFFECTED. ALL COPIES OF 89-121-10 SHOULD BE DISCARDED AND REPLACED BY THIS BULLETIN WHICH INDICATES THE 1989 GEO METRO AS THE INVOLVED MODEL.

The following information covers the top tether anchor installation instructions for rear seat application which was inadvertently omitted from the 1989 GEO Metro Service Manual.

Refer to Installation on next page.

1. Determine location of child restraint seat (left or right).

2. Locate top tether anchor plug(s) and remove.

3. Install top tether anchor assembly with 5/16" bolt and torque to specification.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.