SERVICE MANUAL UPDATE-SEC.7A AUTOMATIC TCM REPLACEMENT. Geo Storm 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC.7A AUTOMATIC TCM REPLACEMENT

#### Subject: AUTOMATIC TRANSAXLE CONTROL MODULE (TCM) REPLACEMENT

#### Model and Year: 1990-91 GEO STORM GSI WITH 4-SPEED AUTOMATIC TRANSAXLE

This bulletin is an amendment to Section 7A of the 1990-91 Geo Storm Service Manuals ST371-90 and ST370-91. Refer to this bulletin for information concerning Transaxle Control Module (TCM) replacement procedures on 1990-91 Geo Storm GSi vehicles equipped with the JF403E 4-speed automatic transaxle.

On-Vehicle Service

Transaxle Control Module (TCM)

Remove or Disconnect

1. Negative (-) battery cable.

2. Switch bezel from instrument panel (pry off with a screwdriver or similar tool) and disconnect electrical connectors from switches.

3. Cigar lighter bezel from instrument panel (pry off with a screwdriver or similar tool) and disconnect cigar lighter electrical connector.

4. Two screws and hood latch release handle from hood latch release cable and knee bolster.

5. Five screws, one nut, one bolt and knee bolster from instrument panel (Figure 1).

6. Two electrical connectors from TCM (Figure 2)

7. Two bolts and TCM from underneath left side of steering column.

Install or Connect

1. TCM to left side of steering column; secure with two bolts.

Tighten

* TCM bolts to 15 N.m (11 lb.ft.).

2. Two electrical connectors to TCM (Figure 2).

3. Knee bolster to instrument panel; secure with one bolt, one nut and five screws.

Tighten

* Knee bolster bolt and nut to 10 N.m (89b.n.).

4. Hood latch release handle to hood latch release cable and knee bolster; secure with two screws.

5. Cigar lighter electrical connector to cigar lighter and cigar lighter bezel into instrument panel.

6. Switch bezel electrical connectors to switches and switch bezel into instrument panel.

7. Negative (-) battery cable.

Tighten

* Negative (-) battery cable-to-negative (-) battery terminal retainer to 15 N.m (11 lb.ft.).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.