SERV. MAN. UPD.-SEC. 7A-1&7A-2 LINE PRESSURE TEST. Geo Storm 1990

For 1990-2009 cars

# SERV. MAN. UPD.-SEC. 7A-1&7A-2 LINE PRESSURE TEST

#### Model and Year: 1990 R CAR

This bulletin is a revision to the line pressure test procedure found in Section 7A-1, page 7A-1-3 and Section 7A-2, page 7A-2-3. Special tool J 25695-10 oil pressure gage adapter must be used in place of J 35752 oil pressure gage adapter shown.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.