SERVICE MANUAL UPDATE-SEC. 7A HIGH CLUTCH HUB SHIM ADJUST. Geo Storm 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 7A HIGH CLUTCH HUB SHIM ADJUST

#### Model and Year: 1990 R CAR

This bulletin is being written to correct the procedure when checking the Oil Pump to High Clutch Hub Shim Adjustment.

Step number 3 on Page 7A2-38 of the 1990 GEO Storm Service Manual should read:

3. Place the J 35284-1 bridge and leg assembly, J 35284-19 bridge extension with J 35284-4 gage cylinder and a J 35284-32 high clutch gage pin on the transaxle case (Figure 132).

The gasket should not be installed when performing this Adjustment.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.