SERVICE MANUAL UPDATE-SEC. 6D3 GENERATOR UNIT REPAIR. Geo Storm 1993

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 6D3 GENERATOR UNIT REPAIR

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6D3 GENERATOR UNIT REPAIR,

#### VEHICLES AFFECTED: 1992-93 "R" MODELS WITH 1.6L ENGINE VIN 6 (RPO L01)

#### APPLICATION:

----------- 1992-93 Geo Storm Models equipped with a VIN 6 1.6L engine (RPO L01)

This bulletin cancels and supersedes the following:

1. VIN 6 generator "Unit Repair" procedure on Page 6D3-4 of the 1992 Geo Storm Service Manual (ST371-92).

2. "Disassembly, Test and Reassembly - VIN 6" procedure on Page 6D3-5 of the 1993 Geo Storm Service Manual (ST371-93).

The generator on a 1992 or 1993 Geo Storm equipped with a VIN 6 engine is now serviceable.

o Whenever service is required to a 1992 Geo Storm equipped with a VIN 6 engine, use the "Generator - VIN 8" procedure on Page 6D3-6 of the 1992 Geo Storm Service Manual (ST371-92).

o Whenever service is required to a 1993 Geo Storm equipped with a VIN 6 engine, use the "Disassembly, Test and Reassembly - VIN 8" procedure on Page 6D3- 7 of the 1993 Geo Storm Service Manual (ST371-93).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.