1992 PAINT CODES, SUPPLIERS, ASSY. PLANT ID-(SERVICE INFO). Geo Tracker - 4WD 1992

For 1990-2009 cars

# 1992 PAINT CODES, SUPPLIERS, ASSY. PLANT ID-(SERVICE INFO)

#### SUBJECT: 1992 PAINT CODES, PAINT SUPPLIERS AND ASSEMBLY PLANT IDENTIFICATION (SERVICE INFORMATION)

#### VEHICLES AFFECTED: 1992 TRUCKS

#### 1992 ASSEMBLY PLANT PAINT IDENTIFICATION

Attached is a current listing of the various assembly plants and their paint suppliers. It should be noted, however, that paint suppliers are subject to change at any given time.

Plant Paint Paint Type Assembly Plant (Trucks) Code Supplier ----------------- ---------------------- ---- ----- Basecoat/Clearcoat Enamel Baltimore, MD (M/L) B PPG High Solids Enamel Janesville, WI (MD) J Dupont High Solids Enamel Lordstown Ohio(G) 7 BASF High Solids Enamel Moraine, OH (S/T) 2 Dupont Basecoat/Clearcoat Waterborne Oshawa Truck Plant (C/K) 1 ICI High Solids Enamel Pontiac-West, MI (S/T) 0 BASF Basecoat/Clearcoat Enamel Pontiac-East, MI (C/K) E Dupont Medium Solids Enamel Scarborough, Ontario (G) 4 ICI High Solids Enamel Shreveport, LA (S/T) 8 BASF Basecoat/Clearcoat Enamel Ft. Wayne, IN (C/K) Z Dupont Basecoat/Clearcoat Enamel Janesville, WI (C/K - J PPG Suburban, Yukon, Sierra Crew Cab)

The following is a list of paint code numbers from various suppliers for the 1992 model year. These colours can be obtained locally.

BASF refinished paints are available in:

A - Alphacryl(R) D - Diamont 88(R) SO-Diamont Solo(R) 21- Glasurit-21(R) 54- Glasurit-54(R) S - Limco Select(R) L - Limco Supreme Gold(R) M - Miracryl(R) Super Max(R)

#### Flexible Finishes

When spraying flexible plastic parts, use the following recommendation:

Elastifier additive 521-111 for Vinyl application when using Glasurit (R) 54 and 21 lines.

891 Flex Agent for Vinyl Application when using Alphacryl(R), Miracryl(R), Diamont 88(R), and Supreme Gold(R).

DF-25 for Vinyl application when using Diamont Solo(R).

#### NOTE: When using a basecoat/clearcoat system only use the flex agent in the clearcoat application.

#### Stone Chip Protector

Glassohyd(TM)1109-1240/6 Stone Chip Protector is a waterborne material which uses a durable, flexible plastic dispersion as its bonding media. This product is versatile in application and may be easily applied by spray, brush, or roller. When Glassohyd(TM)is completely cured, the material is resistant to water, gasoline, and oil. Glassohyd(TM) has excellent stone impact and corrosion resistance. Glassohyd(TM) Stone Chip Protector can be topcoated directly with 21-line or 54/94-line colours.

DuPont refinished paints are available in: -L-Lucite(R)---Acrylic Lacquer -A-Centari(R)---Acrylic Enamel -J-Cronar(R)---Polyoxithane Enamel -K-ChromabaseTM -350S--Flexlar(R) --- Flexible Additive -310S--Black --- 1-2-3 Vinyl Lacquer -330S--White --- 1-2-3 Vinyl Lacquer -V-Lucite Vinyl

#### IMPORTANT: Vinyl resin must be added to the base colour when painting interior components.

DuPont vinyl resin 304S (instrument panel). DuPont vinyl resin 305S (all remaining interior parts except seats). DuPont vinyl resin 306S (seats and vinyl roofs). When ordering DuPont paint, use "L", "A", "J", "K", or "V" with the appropriate DuPont Code.

PPG (Ditzler) refinish paints are available in:

- DDL--Duracryl(R) --- Acrylic Lacquer or Acrylic Basecoat/Clearcoat - DBU--Deltron(R) --- Basecoat/Clearcoat - DAR--Delstar(R) --- Acrylic Enamel - DAU--Deltron(R) --- Acrylic Urethane - UCV --- Vinyl Colours - DX-369--Flexative(R) --- Flexible Finishes - DX-54--Roadguard(R) --- Road Abrasion Protection

When ordering PPG (Ditzler) paint, use "DDL", "DBU", "DAR", "DAU","UCV", "DX-54", or "DX-369" with appropriate Ditzler code.

Sherwin-Williams, Acme/Rogers, and Martin-Senour are available in acrylic lacquer, acrylic enamel, or acrylic urethane.

S-W use: o prefix 34, J4 or L10/L11 for acrylic lacquer, o prefix 35, J5 or F10/F11 for acrylic enamel, o prefix UB for acrylic urethane in a system, o prefix US for acrylic urethane in a single stage system

ACME use: o prefix 84 for acrylic lacquer, o prefix 85 for acrylic enamel, o prefix PB for acrylic urethane in a basecoat/clearcoat system o o prefix PS for acrylic urethane in a single stage system.

Rogers Use: o prefix 94 for acrylic lacquer, o prefix 95 for acrylic enamel, o prefix AU for acrylic urethane in a basecoat/clearcoat system o prefix AS for acrylic urethane in a single stage system.

Martin-Senour: o Jobber will interchange number shown when acrylic lacquer is needed, o use prefix 98 for acrylic urethane as an inter-mix basecoat/clearcoat, o use prefix 88 for acrylic urethane as a factory packaged basecoat/clearcoat, o use prefix 97 for acrylic urethane as an inter-mix single stage system,

#### 1992 TRUCK INTERIOR COLORS

GM Sherwin- Trim Color Name Gloss Fisher Martin- Williams Code Semi Flat W-Code Senour Acme-Rogers ---- ---------- ---- ---- ----- ------ ----------- 13AN Light Gray X 9653 44437 44437 X 44438 44438 13BN Medium Gray X 9654 45940 45940 13CN Dark Gray X 9655 45941 45941 1BDN Dark Charcoal X 7350 17113 34991 X 16851 31901 19DN Black X 16918 33024 X 848 16615 J4-8677 92387 24CN Dark Blue X 36478 36478 X 39838 39838 24DN Very Dark Blue X 8576 17067 34598 X 17075 34606 24EN Midnight Blue X 42600 42600 X 42599 42599 47CN Dark Red X 42602 42602 X 9104 42601 42601 47DN Very Dark Red X 9253 42604 X 42603 60BN Medium Cognac X 9205 38394 38394 X 38393 38393 60CN Dark Cognac X 9099 38395 38395 X 38392 38392 64AN Light Beige X 9776 45942 45942 X 45943 45943 64BN Medium Beige X 9777 45944 45944 45945 45945 64DN Dark Beige X 9778 45946 45946 X 45947 45947

GM PPG PPG Vinyl (BASF) Trim Color Name DIA Interior Rinshed DuPont Code Code UCV Code Mason ---- ----------- ----- -------- ----- ------- 13AN Light Gray 35203 2-1441 21029 C9109 35204 20126 13BN Medium Gray 35205 2-1442 21027 C9110 13CN Dark Gray 35206 2-1443 21028 C9111 1BDN Dark Charcoal 33872 12730 334921 2-871 14030 C8575 19DN Black 9640 4401 9433 120 C8535

24CN Dark Blue 16323 2-1276 17124 C8792 19021 24DN Very Dark Blue 15886 2-1098 15080 C8539 16092 16045 24EN Midnight Blue 16998 2-1396 20065 C9006 16999 20066 47CN Dark Red 73381 2-1394 20061 C9007 73380 20062 47DN Very Dark Red 73383 2-1395 20063 C9008 73382 20064 60BN Medium Cognac 26281 2_1292 18055 C8808 19022 60CN Dark Cognac 26284 2-1315 18056 C8810 18057 64AN Light Beige 2-1477 22275 C9230 27307 22276 64BN Medium Beige 27312 2-1478 22277 C9231 27308 22278 64DN Dark Beige 27313 2-1479 22279 C9232 27309 22280

#### 1992 TRUCK EXTERIOR COLOR

Paint Sherwin- Color Fisher Martin- Williams Code Color Name W-Code DuPont Senour Acme-Rogers --- -------------- ----- ------ ------- ----------- 10 Gray White 9225 B8796 36783 36783 12 Yellow White 5111 817 82-1208 F8W-2030 1492 15 Astral Silver 8914 C8501 82-5915 34856 16 Warm Gray Metallic B/C 9659 B9125 44149 44149 17 Lt. Slate Metallic 7468 B8235 82-5579 32377 19 Lamp Black 5118 99 8800 F10B-1738 80-4080 22 Bahama Blue Met. B/C 9656 B9126 44150 44150 23 Ocean Blue 7154 B8041 82-5258 30527 24 Med. Bright Blue Metallic 9222 B8894 38144 38144 25 Bright Teal 9830 B9224 45877 45877 26 Pastel Blue 9662 B9128 44151 44151 27 Lt. French Blue Metallic 9264 B8944 39337 39337 29 Dark Blue 7349 B8139 82-5448 31514 30 Gray Blue Metallic 9086 B9017 42478 42478 34 Lt. Teal Metallic 9793 B9221 45878 45878 36 Med. Dk. Teal Metailic 9828 B9222 45879 45879 37 Light Mesa Brown 9219 B8897 38147 38147 41 Black B/C 8555 99 82-5760 33756 43 Seafoam Green 9663 B9129 44152 44152 46 Dark Green 7156 B8046 82-5263 30530 47 Dark Blue Metallic 9095 B9019 42479 42479 48 Dark Red 9096 B9020 42480 42480 50 Blue White 8624 B8550 82-5918 34851 51 Sedona Tan 8528 B8542 90-5857 34392 54 Dk. Green Blue Metallic 9831 B9225 45913 45913 57 Beige Metallic 5400 B9213 45881 45881 61 Tan 8265 B8462 82-5799 34070 71 Red Orange 7753 B8250 82-5586 32384 72 Standard Red 7475 B8241 82-5539 32097 74 Victory Red 9260 B8946 39339 39339 75 Red Metallic B/C 8919 C8506 82-5945 34855 76 Dk.Garnet Red Met. B/C 9154 B8742 36454 36454 78 Dark Yellow Red Metallic 8800 B8632 90-6069 35366 90 Gray Metallic 8798 B8629 82-6011 35367 91 Dk. Argent 6270 C9124 45880 45880 94 Blue Red Metallic B/C 9088 B9018 42481 42481 96 Ultra Silver Metailic B/C 8867 B8795 36457 36457 97 Dk. Grey Metallic B/C 9658 B9127 44153 44153 B/C Basecoat/Clearcoat

*M/L Van Only

#### 1992 TRUCK EXTERIOR COLORS

Paint BASF Glasurit Color PPG Rinshed 54-21 Code Color Name DDL-DAR Mason Line ---- ------------ ------- ------- -------- 10 Gray White 4015* 18121 GM-9225 12 Yellow White 2185 1347 GM-5438

15 Astral Silver 3796* 15251 GM-8914 16 Warm Gray Metallic B/C 4314 21017 GM-9659 17 Lt. Slate Metallic 3453 12866 GM-7023 19 Lamp Black 9000/9300 Standard GM-1240 Package 22 Bahama Blue Met. B/C 4307 21018 GM-9656 23 Ocean Blue 3250 11500 GM-5481 24 Med. Bright Blue Metallic 4110 18120 GM-9222 25 Bright Teal 4469 22263 GM-9830 26 Pastel Blue 4308 21019 GM-9662 27 Lt. French Blue Metallic 4146 19031 GM-9264 29 Dark Blue 3362 12283 GM-5039 30 Gray Blue Metallic 4238 20050 GM-9086 34 Lt. Teal Metallic 4455 21040 GM-9793 36 Med. Dk. Teal Metallic 4347 22073 GM-9828 37 Light Mesa Brown 4111 18118 GM-9219 41 Black B/C 9700 13572 54-1240 43 Seafoam Green 4309 21020 GM-9663 46 Dark Green 3255 11505 GM-5482 47 Dark Blue Metallic 4251 20052 GM-9095 48 Dark Red 4239 20053 GM-9096 50 Blue White 3800 15255 GM-8624 51 Sedona Tan 4310 15022 GM-8528 54 Dk. Green Blue Metallic 4500 22267 GM-9831 57 Beige Metallic 4346 22271 GM-5400 61 Tan 3686 14241 GM-1074 71 Red Orange 3463 12884 GM-3046 72 Standard Red 3464 12885 GM-3047 74 Victory Red 4154 19030 GM-9260 75 Red Metallic B/C 3804* 15259 GM-89191 76 Dk. Garnet Red Met. B/C 4002* 21023 GM-9154 78 Dark Yellow Red Metallic 3915 16117 GM-3091 90 Gray Metallic 3916 16118 GM-8798 91 Dk. Argent 34781 22223 GM-22223 94 Blue Red Metallic B/C 4240 20051 GM-9088 96 Ultra Silver Metailic B/C 4023 18112 GM-8867 97 Dk. Grey Metallic B/C 4313 21024 GM-9658 B/C Basecoat/Clearcoat

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.