UPPER DOOR HINGE LOOSENS FROM BODY (PERF. REPAIR PROC.. Geo Tracker - 2WD 1996

For 1990-2009 cars

# UPPER DOOR HINGE LOOSENS FROM BODY (PERF. REPAIR PROC.

#### SUBJECT: UPPER DOOR HINGE LOOSENS FROM BODY (PERFORM REPAIR PROCEDURE USING KIT - TEMPLATE, WELD NUTS)

#### MODELS: 1994-96 GEO TRACKER

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE UPPER DOOR HINGE LOOSENS FROM THE BODY.

#### CORRECTION:

A PROCEDURE HAS BEEN DEVELOPED TO SIMPLIFY THE REPAIR OF THE ABOVE CONDITION. THIS REPAIR REQUIRES THE USE OF A SPECIAL TOOL AND INSTRUCTIONS. KENT MOORE IS THE PROVIDER OF THE REPAIR PACKAGE. THEY CAN BE REACHED BY CALLING 1-800-345-2233 AND REQUESTING PART #J-42237. THIS KIT INCLUDES A TEMPLATE, WELD NUTS, A VIDEO TAPE AND AN INSTRUCTION SHEET. TWO WELD NUTS ARE REQUIRED PER DOOR. THE TOOL AND VIDEO TAPE MUST BE RETURNED TO KENT MOORE AFTER COMPLETION OF THE REPAIR AS THERE ARE NOT ENOUGH TOOLS FOR EVERY DEALERSHIP.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION LABOR OPERATION NUMBER DESCRIPTION TIME --------------- ----------- ---------------

T2320 RH UPPER DOOR HINGE 2.2 HRS

T2321 LH UPPER DOOR HINGE 2.2 HRS

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.