Forward Band Servo Piston Removal. Geo Tracker - 4WD 1997

For 1990-2009 cars

#### Tools Required

J 23075 Third Clutch Servo Piston Spring Compressor

1. Install J 23075 onto the servo piston with the tool offset facing the rear of the transmission case.
2. Compress the servo piston spring (166).
3. Remove the servo piston retainer ring (167).
4. Slowly release the pressure on the servo piston assembly (166).
5. Remove J 23075 .
6. Remove the servo piston assembly (166).
7. Remove the return spring (156).
8. The servo apply rod (157).
9. Inspect the servo apply rod for:

• | nicks

• | burrs

• | scoring