ASSY PLANT IDENTIFICATION AND PAINT SUPPLIERS. Geo Tracker - 2WD 1991

For 1990-2009 cars

# ASSY PLANT IDENTIFICATION AND PAINT SUPPLIERS

#### Subject: PAINT CODES, ASSEMBLY PLANT IDENTIFICATION AND PAINT SUPPLIERS

#### Model and Year: ALL 1991 TRUCKS

This Bulletin is being revised to change the Sherwin-Williams Acme Rogers Exterior Colour Code for Paint Colour Code 44 (Forest Green Metallic) 35441 on the colour chart.

The following is a list of paint code numbers from various suppliers for the 1991 model year. These colors can be obtained locally.

BASF refinished paints are available in:

A - Alphacryl

D - Diamont 88

SO-Diamont Solo

21 - Glasurit-21

54- Glasurit-54

S - Limco Select

L - Limco Supreme Gold

M - Miracryl

- Super Max

Flexible Finishes

When spraying flexible plastic parts, use the following recommendation:

Elastifier additive 521-111 for Vinyl application when using Glasurit 54 and 21 lines.

891 Flex Agent for Vinyl Application when using Alphacryl, Miracryl, Diamont 88, and Supreme Gold.

DF-25 for Vinyl application when using Diamont Solo.

#### NOTE: When using a basecoat/clearcoat system only use the flex agent in the clearcoat application.

#### Stone Chip Protector

Glassohyd TM 1109-1240/6 Stone Chip Protector is a waterborne material based on a durable, flexible plastic dispersion as its bonding media. This product is versatile in application and may be easily applied by spray, brush, or roller. When Glassohyd TM is completely cured, the material is resistant to water, gasoline, and oil. Glassohyd YM has excellent impact and corrosion resistance. Glassohyd TM 1109-1240/6 Stone Chip Protector can be topcoated directly with 21-line or 54/94-line colors.

DuPont refinished paints are available in:

- L-Lucite-Acrylic Lacquer

- A-Centari-Acrylic Enamel

-J-Cronar-Polyoxithane Enamel

-K-Chromabase

-35OS-Flexlar - Flexible Additive

-310S-Black-1-2-3 Vinyl Lacquer

-330S-White-1-2-3 Vinyl Lacquer

-Lucite Vinyl

#### IMPORTANT: Vinyl resin must be added to the base color when painting interior components.

DuPont vinyl resin #304 instrument panel

DuPont vinyl resin #305 all remaining interior parts except seats.

DuPont vinyl resin #306 seats and vinyl roofs.

When ordering DuPont paint, use "L," "A," "J," "K," "V," 350S or 1-2-3 White or 1-2-3 Black with the appropriate DuPont Code.

PPG (Ditzler) refinish paints are available in:

- DDL-Duracryl-Acrylic Lacquer or Acrylic Basecoat/Clearcoat

- DBU-Deltron-Basecoat/Clearcoat

- DAR-Delstar-Acrylic Enamel

- DAU-Deltron-Acrylic Urethane

- UCV-Vinyl Colors

- DX-369-Flexative-Flexible Finishes

- DX-54-Roadguard-Road Abrasion Protection

When ordering PPG (Ditzler paint, use "DDL," "DBU," "DAR," "DAU," "UCV," "DX-54," "DX- 369" with appropriate Ditzler code.

Sherwin-Williams, Acme/Rogers, and Martin-Senour are available in acrylic lacquer, acrylic enamel, or acrylic urethane.

S-W use: prefix 34, J4 or L10 for acrylic lacquer, prefix 35, J5 or F10 for acrylic enamel, prefix UB for acrylic urethane in a basecoat/clearcoat system, prefix US for acrylic urethane in a single stage system.

ACME use: prefix 84 for acrylic lacquer, prefix 85 for acrylic enamel, prefix PB for acrylic urethane in a basecoat/clearcoat system prefix PS for acrylic urethane in a single stage system.

Rogers Use: prefix 94 for acrylic lacquer, prefix 95 for acrylic enamel, prefix AU for acrylic urethane in a basecoat/clearcoat system, prefix AS for acrylic urethane in a single stage system.

Martin-Senour: Jobber will interchange number shown when acrylic lacquer is needed, use prefix 98 for acrylic urethane as a pre-mix basecoat/clearcoat, use prefix 88 for acrylic urethane as a factory packaged basecoat/clearcoat, use prefix 97 for acyrlic urethane as a pre-mix single stage system, use prefix 87 for acrylic urethane as a factory packaged single stage system.

#### 1991 ASSEMBLY PLANT PAINT IDENTIFICATION

Plant Paint Paint Type, Assembly Plant Trucks Code Supplier ----------------- ---------------------- ---- -------- Basecoat/Clearcoat Baltimore, MD (M Vans) B PPG Enamel Basecoat/Clearcoat Flint, MI (Suburban and F BASF Enamel utility) High Solids Enamel Janesville, WI (MD Truck and C/K) J Dupont High Solids Enamel Lordstown, OH (G Van) 7 BASF High Solids Enamel Moraine, OH (S/T Truck) 2 BASF Basecoat/Clearcoat Oshawa Truck Plant (C/K) 1 ICI Waterborne High Solids Enamel Pontiac-West, MI (S/T) 0 BASF Basecoat/Clearcoat Pontiac-East, MI (C/K) E Dupont Enamel Medium Solids Enamel Scarborough, Ontario (G Van) 4 ICI High Solids Enamel Shreveport, LA (S Truck) 8 BASF Basecoat/Clearcoat Ft. Wayne, IN (C/K Truck) Z Dupont High Solids Enamel Flint, MI (R/V Truck) F BASF

#### 1991 TRUCK EXTERIOR COLORS

Paint Color Fisher Martin- PPG Code Color Name W-Code DuPont Senour DDL-DAR

10 White B/C 9225 B8796 36783 4015* 12 White 5111 817 82-1208 2185

15 Silver Metallic B/C 8914 C8501 82-5915 3796* 16 Warm Gray Metallic B/C 9659 B9125 44149 4314 17 Slate Metallic 7468 B8235 82-5579 3453 19 Black 5118 99 8800 9000/9300

22 Bahama Blue Met. B/C 9656 B9126 44150 4307 23 Medium Blue 7154 B8041 82-5258 3250 24 Bright Blue Metallic 9222 B8894 38144 4110 26 Pastel Blue 9662 B9128 44151 4308 27 Lt. Blue Metallic B/C 9264 B8944 39337 4146 29 Dark Blue 7349 88139 82-5448 3362 30 Med. Blue Metallic B/C 9086 89017 42478 4238 33 Light Mesa Brown B/C 9207 B8945 39338 4152 34 Lt. Mesa Brown Met. B/C 9208 B8895 38145 4107 37 Light Mesa Brown 9219 B8897 38147 4111 41 Black B/C 8555 99 82-5760 9700 42 Sky Blue 9203 B8943 40381 16813 43 Seafoam Green 9663 B9129 44152 4309 44 Forest Green Metallic 7964 D8801 82-6024 4114 46 Woodland Green 7156 B8046 82-5263 3255 47 Dark Blue Metallic B9019 42479 4251 48 Dark Red 9096 B9020 42480 4239 50 White B/C 8624 B8550 82-5918 3800 51 Sedona Tan 8528 B8542 90-5857 4310 58 Lt. Sandstone Metallic B/C 8865 B8792 36450 4020 61 Tan 8265 B8462 82-5799 3686 70 Red B/C 8832 B8793 36453 4021 7 1 Red Orange 7753 B8250 82-5586 3463 72 Bright Red 7475 B8241 82-5539 3464 74 Red B/C 9260 B8946 39339 4154 75 Red Metallic B/C 8919 C8506 82-5945 3804* 77 Dk. Garnet Red Met. B/C 9154 B8742 36454 4002* 78 Dark Maple Metallic 8800 B8632 90-6069 3915 86 Wheatland Yellow 9418 B9044 43350 88 Tangier Orange 9417 B9045 43349 90 Gray Metallic 8798 B8629 82-6011 3916 94 Red Metallic B/C 9088 B9018 42481 4240 96 Silver Metallic B/C 8867 B8795 36457 4023 97 Dk. Grey Metallic B/C 9658 B9127 44153 4313 98 Black Sapphire Metallic B/C 8863 B8745 36458 4003

B/C Basecoat/Clearcoat

'M Van Only

Paint BASF Glasurit Color Sherwin-Williams Rinshed 54-21 Code Color Name Acme-Rogers Mason Line --- ------------ ----------------- ------- --------- 10 White B/C 36783 18121 GM-9225 12 White F8W-2030 1347 GM-5438 1492 15 Silver Metallic B/C 34856 15251 GM-7054 16 Warm Gray Metallic B/C 44149 21017 GM-9659 17 Slate Metallic 32377 12866 GM-7023 19 Black F10B-1738 Standard GM-1240 80-4080 Package 22 Bahama Blue Met. B/C 44150 21018 GM-9656 23 Medium Blue 30527 11500 GM-5481 24 Bright Blue Metallic 38144 18120 GM-9222 26 Pastel Blue 44151 21019 GM-9662 27 Lt. Blue Metallic B/C 39337 19031 GM-9264 29 Dark Blue 31514 12283 GM-5039 30 Med. Blue Metallic B/C 42478 20050 GM-9086 33 Light Mesa Brown B/C 39338 19028 GM-9207 34 Lt. Mesa Brown Met. B/C 38145 18116 GM-9208 37 Light Mesa Brown 38147 18118 GM-9219 41 Black B/C 33756 13572 54-1240 42 Sky Blue 40381 19027 GM-9203 43 Seafoam Green 44152 - GM-9663 44 Forest Green Metallic 35441 15366 GM-7964 46 Woodland Green 30530 11505 GM-5482 47 Dark Blue Metallic 42479 20052 GM-9095 48 Dark Red 42480 20053 GM-9096 50 White B/C 34851 15255 GM-8624 51 Sedona Tan 34392 15022 GM-8528 58 Lt. Sandstone Metallic B/C 36450 18111 GM-8865 61 Tan 34070 14241 GM-1074 70 Red B/C 36453 18115 GM-8332 7 1 Red Orange 32384 12884 GM-3046 72 Bright Red 32097 12885 GM-3047 74 Red B/C 39339 19030 GM-9260 75 Red Metallic B/C 34855 15259 GM-89191 77 Dk. Garnet Red Met. B/C 36454 21023 GM-9154 78 Dark Maple Metallic 35366 16117 GM-3091 86 Wheatland Yellow 43350 21025 GM-9418 88 Tangier Orange 43349 21021 GM-9417 90 Gray Metallic 35367 16118 GM-8798 94 Red Metallic B/C 42481 20051 GM-9088 96 Silver Metallic B/C 36457 18112 GM-8867 97 Dk Grey Metallic B/C 44153 21024 GM-9658 98 Black Sapphire Metallic B/C 36458 17118 GM-8863

1991 TRUCK INTERIOR COLORS

Sherwin- GM Gloss Fisher Martin- Williams Trim Color Name W-Code Senour Code Semi Flat Acme-Rogers ---- ---------------- ------------ ----- ------- ----------- 13AN Light Gray x 9653 44437 44438 X 44438 44437 13BN Medium Gray x 9654 44439 44439 13CN Dark Gray X 9655 44440 44440 18DN Dark Charcoal x 7350 17113 34991 x 16851 31901 19DN Black x 16918 33024 x 848 16615 J4-8677 92387 23DN Dark Blue X 7163 16742 30821 24CN Dark Blue x 9059 36478 36478 39838 39838 24DN Very Dark Blue x 8576 17067 34598 x 17075 34606 24EN Midnight Blue x 9541 42600 42600 x 42599 42599 47CN Dark Red x 9104 42602 42602 x 42601 42601 47DN Very Dark Red x 9253 42604 42604 x 42603 42603 60BN Medium Cognac x 9205 38394 38394 x 38393 38393 60CN Dark Cognac x 9099 38395 38395 x 38392 38392 60DN Very Dark Cognac 9252 38391 38391 69BN Medium Beige x 8248 16950 33715 x 16966 33770 69CN Medium Dark Beige x 828 17066 34597 x 17074 34605

GM PPG PPG Vinyl (BASF) Trim Color Name DIA Interior Rinshed DuPont Code Code UCV Code Mason

13AN Light Gray 35203 2-1441 21029 C9109 35204 13BN Medium Gray 35205 2-1442 21027 C9110 13CN Dark Gray 35206 2-1443 21028 C9111 18DN Dark Charcoal 33872 2-871 12730 33492 14030 C8575 19DN Black 9640 4401 9433 120 12812 C8535

23DN Dark Blue 15392 2-765 11595 C8002 24CN Dark Blue 16323 2-1276 17124 C8792 19021 24DN Very Dark Blue 15886 2-1098 15080 C8539 16092 16045 24EN Midnight Blue 16998 2-1396 20065 C9006 16999 20066 47CN Dark Red 73381 2-1394 20061 C9007 73380 20062 47DN Very Dark Red 73383 2-1395 20063 C9008 73382 20064 26281 18055 60CN Medium Cognac -- 2-1292 C8808 19022 60CN Dark Cognac 26284 2-1315 18056 C8810 - 18057 60DN Very Dark Cognac 26285 2-1316 18059 C8819 69BN Medium Beige 25313 2-1045 14006 C8446 - 20060 69CN Medium Dark Beige 25514 2-1117 17120 C8554 25571 15065

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.