SMU - SECTIONS 8A 10/11/47 - POWER DISTRIBUTION, FUSE BLOCK. Geo Tracker - 2WD 1997

For 1990-2009 cars

# SMU - SECTIONS 8A 10/11/47 - POWER DISTRIBUTION, FUSE BLOCK

#### SUBJECT: SERVICE MANUAL UPDATE - SECTIONS 8A-10/11/47 - POWER DISTRIBUTION, FUSE BLOCK DETAILS, SIR - REVISED SCHEMATICS (SIR IG FUSE)

#### MODELS: 1996-97 GEO TRACKER

THIS BULLETIN IS BEING ISSUED TO REVISE THE SCHEMATICS IN SECTIONS 8A-10 (POWER DISTRIBUTION), 8A-11 (FUSE BLOCK DETAILS) AND 8A-47 (SUPPLEMENTAL INFLATABLE RESTRAINT) OF THE SERVICE MANUAL.

THE CHANGE ON THE SCHEMATICS IS THE POWER FEED TO THE SIR IG FUSE. THE FUSE IS TIED TO THE ON AND START POSITIONS OF THE IGNITION SWITCH, MAKING THE FUSE HOT IN ON AND START.

PLEASE USE THE ATTACHED SCHEMATICS TO REPLACE THE EXISTING ONES IN THE APPROPRIATE SECTIONS OF THE SERVICE MANUAL.

FIGURES: 00 ATTACHMENTS: 03

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.