Evaporative Emission Tank Pressure Control Solenoid Valve Replace. Geo Tracker - 2WD 1997

For 1990-2009 cars

### Removal Procedure

1. Disconnect the EVAP tank pressure control solenoid vacuum valve electrical connector (4).
2. Disconnect the two vacuum hoses (1) from the EVAP tank pressure control solenoid vacuum valve.
3. Remove the screw (2) and the EVAP tank pressure control solenoid vacuum valve (3) from the RH inner fender bracket.

### Installation Procedure

1. Install the EVAP tank pressure control solenoid vacuum valve (3) to the RH inner fender bracket.
2. Secure the EVAP tank pressure control solenoid vacuum valve with the one screw (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Tighten the EVAP tank pressure control solenoid vacuum valve screw.

Tighten
Tighten the screw to 10 N·m (89 lb in).

4. Connect the two vacuum hoses (1) to the EVAP tank pressure control solenoid vacuum valve.
5. Connect the EVAP tank pressure control solenoid vacuum valve electrical connector (4).