Engine Controls Components. Geo Tracker - 4WD 1996

For 1990-2009 cars

Name | Location
--- | ---
A/C Amplifier | Behind RH I/P on Evaporator
Camshaft Position Sensor | Inside the distributor, at the rear of the engine
Clutch Pedal Position (CPP) Switch (Manual Transmission) | Behind LH I/P, above Powertrain Control Module (PCM)
Crankshaft Position Sensor | Lower front of the Engine, front of the Oil Pan
Data Link Connector (DLC) | LH I/P, Left of Center Console on Knee Bolster
Distributor | Top rear of Engine
Duty Check Data Link Connector (DLC) 1 | RH Engine Compartment, behind RH Headlamp
Engine Control Module (ECM) / Powertrain Control Module (PCM) | Under LH I/P, left of Steering Column
Evaporative (EVAP) Canister Purge Valve | RH front Engine, on Intake Manifold
Evaporative (EVAP) Canister Vent Control Valve, 4-door only | RH Engine Compartment, near Fuse Block1
Evaporative (EVAP) Tank Pressure Control Solenoid Vacuum Valve, 4-door only | RH Engine Compartment, near Fuse Block 1
Exhaust Gas Recirculation (EGR) Bypass Valve | RH front engine, on intake manifold
Exhaust Gas Recirculation (EGR) Solenoid Vacuum Valve | RH front Engine, on Intake Manifold
Fuel Injector #1 | Top RH side of Engine
Fuel Injector #2 | Top RH side of Engine
Fuel Injector #3 | Top RH side of Engine
Fuel Injector #4 | Top RH side of Engine
Fuel Level Sensor | In Fuel Tank
Fuel Pump | In Fuel Tank
Fuel Pump Relay | Center I/P, behind Blower Speed Selector Switch
Fuel Tank Pressure Sensor, 4-door only | On top of fuel tank
Fuse Block 1 | LH engine compartment mounted on the LH inner fender behind the relay box
Fuse Block 1 - C1 (3 Cavities) | Main Harness to Fuse Block 1, below Fuse Block 1
Fuse Block 2 | Under LH I/P
Generator | RH Lower front of Engine
Heated Oxygen Sensor 1 (HO2S1) | LH rear of Engine, in Exhaust Manifold
Heated Oxygen Sensor 2 (HO2S2) | Below Vehicle after Three-Way Catalytic Converter (TWC)
Idle Air Control (IAC) Valve | RH Engine, below Throttle Body
Ignition Control Module | Inside the distributor, rear of the engine
Ignition Coil | Inside the distributor, rear of the engine
Ignition Switch | On Steering Column
Intake Air Temperature (IAT) Sensor | LH front of the engine, in the air cleaner housing
Instrument Panel Cluster Assembly | LH I/P
Junction Connector 2 (20 Cavities) | IP harness, LH side of the IP, behind the illumination controller center IP, behind the blower speed selector switch
Manifold Absolute Pressure (MAP) Sensor | Rear Engine Compartment, on Bulkhead
Mass Air Flow (MAF) Sensor | LH Front Engine compartment, on Air Cleaner (ACL) Housing
Noise Suppressor Filter | LH Front Engine Compartment, below Front Wiper Motor
Park/Neutral Position (PNP) Switch (3-Speed Automatic transmission) | RH side of Transmission
Starter Motor | Lower RH side of Engine, under Intake Manifold
Stoplamp Switch | Under LH I/P, above Brake Pedal
Throttle Position (TP) Sensor | On Throttle Body