SMU - SECTIONS 0B & 6D - REVISED SPARK PLUG USAGE. Geo Tracker - 2WD 1995

For 1990-2009 cars

# SMU - SECTIONS 0B & 6D - REVISED SPARK PLUG USAGE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTIONS 0B AND 6D - REVISED SPARK PLUG USAGE INFORMATION

#### MODELS: 1995-97 GEO TRACKER WITH 1.6L ENGINE (VINS U, 6 - RPOS LS5, L01)

THIS BULLETIN IS BEING ISSUED TO REVISE THE SPARK PLUG USAGE INFORMATION FOUND IN THE "MAINTENANCE AND LUBRICATION" AND "IGNITION SYSTEM" SECTIONS OF THE 1995-97 SERVICE MANUALS.

1995 ====

1.6L (VIN U):

SPARK PLUGS AND GAP AC TYPE R43XLS (GM P/N 5613522) . . . . . . . . . . . . 0.7-0.8MM (0.028-0.032 IN)

1.6L (VIN 6):

SPARK PLUGS AND GAP NGK TYPE BKR6E (GM P/N 96068562). . . . . . . . . . . . 0.7-0.8MM (0.028-0.032 IN)

NIPPONDENSO TYPE K20PR-U (GM P/N 96068563). . . . . . . 0.7-0.8MM (0.028-0.032 IN)

1996-1997 =========

1.6L (VIN 6):

SPARK PLUGS AND GAP NGK TYPE BKR6E (GM P/N 96068562). . . . . . . . . . . . 0.7-0.8MM (0.028-0.032 IN)

NIPPONDENSO TYPE K20PR-U (GM P/N 96068563). . . . . . . 0.7-0.8MM (0.028-0.032 IN)

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.