Forward Band Servo Piston Installation. Geo Tracker - 2WD 1997

For 1990-2009 cars

#### Tools Required

• | J 38428 Servo Piston Ring Sleeve

• | J 23075 Servo and Clutch Piston Compressor

1. Install the servo apply rod (157). The round end goes into the case.
2. Install the servo piston return spring (156).
3. Install J 38428 over the servo piston.
4. Place the servo piston into the transmission case.
5. Install J 23075 . The tool offset faces toward the rear of the case.
6. Compress the servo piston return spring.
7. Remove J 38428 .
8. Install the servo piston retainer ring (167).
9. Remove J 23075 .