TOWING PROCEDURES FOR THE 1990 GEO TRACKER LSI. Geo Tracker - 4WD 1990

For 1990-2009 cars

# TOWING PROCEDURES FOR THE 1990 GEO TRACKER LSI

#### Model and Year: 1990 (GEO TRACKER LSI) J1 TRUCK

The 1990 GEO Tracker LSI Front Towing Procedures are the same as for the 1990 GEO Tracker, except dollies MUST BE USED under rear wheels.

The 1990 GEO Tracker LSI rear towing procedures are the same as for the 1990 GEO Tracker.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.