SERVICE MANUAL UPDATE FRONT WHEEL BEARINGS TORQUE. Geo Tracker - 4WD 1989

For 1990-2009 cars

# SERVICE MANUAL UPDATE FRONT WHEEL BEARINGS TORQUE

#### Model and Year: 1989 GEO TRACKER

#### TO: ALL CHEVROLET DEALERS

This bulletin is being written to correct the Wheel Bearing Torque printed on page 3C-9 of the 1989 GEO Tracker service Manual. The torque value printed below should be used when tightening the Front Wheel Bearing Lock Nut.

Front Wheel Bearing 170 - 250 N.m (123 - 180 lbs. ft.)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.