For 1990-2009 cars

### Removal Procedure

1. Disconnect the hood release cable from the hood latch release handle.
2. Remove the I/P undercover.
3. Remove the driver side knee bolster.
4. Disconnect the tire pressure module connector.
5. Remove the tire pressure module retaining screws and the module (1).

### Installation Procedure

1. Install the tire pressure module (1). Secure with retaining screws.
2. Connect the tire pressure module connector.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the driver side knee bolster.

Tighten
Tighten the knee bolster bolts to 10 N·m (89 lb in).

4. Install the I/P undercover.
5. Connect the hood release cable to the hood latch release handle.