For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the crankshaft position (CKP) sensor connector (1).
3. Remove the CKP sensor retaining bolt.
4. Remove the CKP sensor.

### Installation Procedure

1. Install the CKP sensor.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the CKP sensor retaining bolt and tighten to 6.5 N·m (58 lb in).
3. Connect the crankshaft position (CKP) sensor connector (1).
4. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.