For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the T-MAP sensor connector.
3. Remove the T-MAP sensor retaining bolt.
4. Remove the T-MAP sensor (1).

### Installation Procedure

1. Install the T-MAP sensor (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the T-MAP sensor retaining bolt and tighten to 10 N·m (89 lb in).
3. Connect the T-MAP sensor connector.
4. Connect the negative battery cable.