For 1990-2009 cars

### Removal Procedure

Notice: Refer to Vehicle Lifting and Jacking Notice in the Preface section.

1. Raise and support the vehicle.
2. Disconnect the brake line from the brake hose support bracket on the wheel housing.
3. Remove the E-ring retainer.
4. Remove the brake hose from the wheelhousing bracket.
5. Remove the bolt from the brake caliper.
6. Remove the seal rings and the brake hose.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the new brake hose to the caliper with new seal rings and the bolt.

Tighten
Tighten the front brake hose-to-caliper bolt to 40 N·m (30 lb ft).

2. Install the brake hose and the E-ring retainer to the wheelhousing bracket.
3. Connect the brake line to the brake hose.

Tighten
Tighten the brake line to 16 N·m (12 lb ft).

4. Lower the vehicle.
5. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .
6. Check the brake system for leaks.