For 1990-2009 cars

### Removal Procedure

1. Mark the clutch release arm location to the release shaft position.
2. Remove the adjusting nut (1) for the clutch cable.
3. Remove the clutch control cable (2) from the release arm.
4. Remove the clutch release am retaining bolt and nut (1).
5. Remove the release arm (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the release arm to the release shaft and align to the marked position (1).
2. Install the release arm bolt and nut and tighten to 16 N·m (12 lb ft).
3. Install the clutch control cable to the release arm and install the clutch control cable adjusting nut.
4. Adjust the clutch cable. Refer to Clutch Assembly Adjustment.