For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Disconnect the windshield washer hose from the washer nozzles on the hood.
3. Remove the front left wheel. Refer to Tire and Wheel Removal and Installation .
4. Remove the bolts and the front wheel well splash shield.
5. Disconnect the washer hose from the washer reservoir.

### Installation Procedure

1. Route the washer hose to the washer reservoir.
2. Connect the washer hose to the washer reservoir.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front wheel well splash shield with the bolts.

Tighten
Tighten the front wheel well splash shield bolts to 1.5 N·m (13 lb in).

4. Install the front left wheel. Refer to Tire and Wheel Removal and Installation .
5. Connect the windshield washer hose to the washer nozzles on the hood.
6. Close the hood.