For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the door seal trim. Refer to Door Water Deflector Replacement.
3. Remove the outside channel molding. Refer to Front Side Door Window Channel Replacement.
4. Remove the screws that secure the glass to the window regulator.
5. Remove the bolts and the guide rail.
6. Remove the glass from the door.

### Installation Procedure

1. Install the glass in the door.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the guide rail and the bolts. Tighten the guide rail bolts to 7 N·m (62 lb in).
3. Install the glass to the window regulator with the screws. Tighten the door glass screws to 7 N·m (62 lb in).
4. Install the outside channel molding. Refer to Front Side Door Window Channel Replacement.
5. Install the door seal trim. Refer to Door Water Deflector Replacement.
6. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement.