For 1990-2009 cars

#### Tools Required

J 28467-B (DW-117) Universal Engine Support Fixture

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Support the engine assembly using the J 28467-B .
3. Remove the engine mount bracket attaching bolts/nuts.
4. Remove the front timing belt cover. Refer to Timing Belt Cover Replacement .
5. Remove the engine mount attaching bolts/nuts.
6. Remove the engine mount.

### Installation Procedure

1. Install the engine mount.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the engine mount retaining bolts.

Tighten
Tighten the engine mount attaching bolts to 30 N·m (22 lb ft).

3. Install the front timing belt cover. Refer to Timing Belt Cover Replacement .
4. Install the engine mount bracket attaching bolts/nuts.

Tighten
Tighten the engine mount bracket attaching bolts/nuts to 55 N·m (41 lb ft).

5. Remove the J 28467-B .
6. Connect the negative battery cable.