For 1990-2009 cars

### Removal Procedure

1. Disconnect the vehicle speed sensor (VSS) connector (1).

Caution: In order to avoid being burned, do not service the exhaust system while it is still hot. Service the system when it is cool.

2. Remove the bolt and the speedometer driven gear assembly.
3. Remove the VSS (1) from the speedometer driven gear (2).

### Inspection Procedure

1. Remove the O-ring (2) from the speedometer driven gear housing.
2. Remove the driven gear pin (1) and disconnect the driven gear (3).
3. Inspect for a damaged or torn O-ring.
4. Inspect for a worn or damaged tooth on the driven gear.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the speedometer driven gear assembly (2) to the transaxle housing mounting bolt.

Tighten
Tighten the bolt to 5-8 N·m (44-71 lb in).

2. Connect the VSS connector.