For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Accelerator Pedal Nut | 12 N·m | 106 lb in
Camshaft Position Actuator Solenoid Valve Bolt | 6 N·m | 53 lb in
Crankshaft Position (CKP) Sensor Bolt | 4.5 N·m | 40 lb in
Engine Control Module (ECM) Nuts | 8 N·m | 71 lb in
Engine Coolant Temperature 2 (ECT2) Sensor | 20 N·m | 15 lb ft
Fuel Filter Bracket Bolt | 4 N·m | 35 lb in
Fuel Rail Bolt | 8 N·m | 71 lb in
Heated Oxygen Sensor (HO2S) | 40 N·m | 30 lb ft
Ignition Coil Bolt | 8 N·m | 71 lb in
Knock Sensor (KS) Bolt | 20 N·m | 15 lb ft
Map Sensor Screw | 8 N·m | 71 lb in
Throttle Body Bolts | 8 N·m | 71 lb in