For 1990-2009 cars

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B1101 | Battery Voltage High | SDM | DTC B1101
B1102 | Battery Voltage Low | SDM | DTC B1102
B1103 | SIR Serial Communications Fault | SDM | DTC B1103
B1104 | Passenger Seat Occupant Classification System (OCS) Voltage Out of Range | SDM | DTC B1104
B1326 | Front End Sensor 1 Short to Ground | SDM | DTC B1326
B1327 | Front End Sensor 1 Short to Battery | SDM | DTC B1327
B1328 | Front End Sensor 1 Internal Electronic Failure | SDM | DTC B1328
B1329 | Front End Sensor 1 Invalid Serial Data Received | SDM | DTC B1329
B1330 | Incorrect Electronic Front End Sensor 1 Installed | SDM | DTC B1330
B1331 | Front End Sensor 2 Short to Ground | SDM | DTC B1331
B1332 | Front End Sensor 2 Short to Battery | SDM | DTC B1332
B1333 | Front End Sensor 2 Internal Electronic Failure | SDM | DTC B1333
B1334 | Front End Sensor 2 Invalid Serial Data Received | SDM | DTC B1334
B1335 | Incorrect Electronic Front End Sensor 2 Installed | SDM | DTC B1335
B1346 | Driver Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1346
B1347 | Driver Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1347
B1348 | Driver Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1348
B1349 | Driver Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1349
B1352 | Passenger Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1352
B1353 | Passenger Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1353
B1354 | Passenger Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1354
B1355 | Passenger Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1355
B1361 | Driver Pretensioner Deployment Loop Resistance High | SDM | DTC B1361
B1362 | Driver Pretensioner Deployment Loop Resistance Low | SDM | DTC B1362
B1363 | Driver Pretensioner Deployment Loop Short to Ground | SDM | DTC B1363
B1364 | Driver Pretensioner Deployment Loop Short to Battery | SDM | DTC B1364
B1367 | Passenger Pretensioner Deployment Loop Resistance High | SDM | DTC B1367
B1368 | Passenger Pretensioner Deployment Loop Resistance Low | SDM | DTC B1368
B1369 | Passenger Pretensioner Deployment Loop Short to Ground | SDM | DTC B1369
B1370 | Passenger Pretensioner Deployment Loop Short to Battery | SDM | DTC B1370
B1378 | LF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1378
B1379 | LF Side Deployment Loop Resistance Low | SDM | DTC B1379
B1380 | LF Side Deployment Loop Short to Ground | SDM | DTC B1380
B1381 | LF Side Deployment Loop Short to Battery | SDM | DTC B1381
B1382 | RF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1382
B1383 | RF Side Deployment Loop Resistance Low | SDM | DTC B1383
B1384 | RF Side Deployment Loop Short to Ground | SDM | DTC B1384
B1385 | RF Side Deployment Loop Short to Battery | SDM | DTC B1385
B1395 | Deployment Loops Interconnect Circuit | SDM | DTC B1395
B1400 | Driver SIS Malfunction | SDM | DTC B1400
B1401 | LF Side Impact Sensor Short to Ground | SDM | DTC B1401
B1402 | LF Side Impact Sensor Short to Battery | SDM | DTC B1402
B1403 | Passenger SIS Malfunction | SDM | DTC B1403
B1404 | RF Side Impact Sensor Short to Ground | SDM | DTC B1404
B1405 | RF Side Impact Sensor Short to Battery | SDM | DTC B1405
B1409 | LF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1409
B1410 | RF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1410
B1414 | LF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1414
B1415 | RF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1415
B1440 | Passenger Seat Occupant Classification System (OCS) Short to Ground | SDM | DTC B1440
B1446 | Passenger Seat Occupant Classification System (OCS) Short to Battery | SDM | DTC B1446
B1447 | Passenger Seat Occupant Classification System (OCS) Sensor Circuit | SDM | DTC B1447
B1448 | Passenger Seat Occupant Classification System (OCS) Sensor | SDM | DTC B1448
B1449 | Passenger Seat Occupant Classification Sensor Communication | SDM | DTC B1449
B1450 | Incorrect Passenger Seat Occupant Classification Sensor Installed | SDM | DTC B1450
B1481 | Driver Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1481
B1482 | Driver Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1482
B1483 | Driver Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1483
B1484 | Driver Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1484
B1485 | Passenger Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1485
B1486 | Passenger Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1486
B1487 | Passenger Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1487
B1488 | Passenger Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1488
B1620 | ECU Performance | SDM | DTC B1620
B1650 | Frontal Stage 1 Deployment Commanded | SDM | DTC B1650
B1651 | LH Side Air Bag Deployment Commanded | SDM | DTC B1651
B1652 | RH Side Air Bag Deployment Commanded | SDM | DTC B1652
B1657 | Deployment Commanded Pretensioner | SDM | DTC B1657
B1670 | Frontal Stage 2 Deployment Commanded | SDM | DTC B1670
B2500 | Inflatable Restraint System Indicator Circuit | SDM | DTC B2500
B2501 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2501
B2502 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2502
C1101 | Battery Voltage High | EBCM | DTC C1101
C1102 | Left Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1102
C1200 | Left Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1200
C1201 | Left Front Wheel Speed Circuit Range Performance | EBCM | DTC C1201
C1202 | Left Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1202
C1203 | Right Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1203
C1204 | Right Front Wheel Speed Circuit Range Performance | EBCM | DTC C1204
C1205 | Right Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1205
C1206 | Left Rear Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1206
C1207 | Left Rear Wheel Speed Sensor Circuit Range Performance | EBCM | DTC C1207
C1208 | Left Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1208
C1209 | Right Rear Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1209
C1210 | ECU Malfunction | EBCM | DTC C1210
C1211 | Right Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1211
C1604 | ECU Malfunction | EBCM | DTC C1604
C2112 | Solenoid Valve Relay Circuit | EBCM | DTC C2112
C2402 | Pump Motor Circuit | EBCM | DTC C2402
P0016 | Camshaft Position (CMP) Sensor Performance | ECM | DTC P0016 or P0340
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM | DTC P0030 or P0036
P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038
P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM | DTC P0030 or P0036
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038
P0068 | Throttle Body Air Flow Performance | ECM | DTC P0068
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM |

• | DTC P0106 for the 1.4L DOHC engine

• | DTC P0106 for the 1.4L SOHC engine

• | DTC P0106 for the 1.6L engine

P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM |

• | DTC P0107 or P0108 for the 1.2L engine

• | DTC P0107 or P0108 for the 1.4L DOHC engine

• | DTC P0107 or P0108 for the 1.4L SOHC engine

• | DTC P0107 or P0108 for the 1.5L engine

• | DTC P0107 or P0108 for the 1.6L engine

P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM |

• | DTC P0107 or P0108 for the 1.2L engine

• | DTC P0107 or P0108 for the 1.4L DOHC

• | DTC P0107 or P0108 for the 1.4L SOHC engine

• | DTC P0107 or P0108 for the 1.5L engine

• | DTC P0107 or P0108 for the 1.6L engine

P0110 | Intake Air Temperature (IAT) Sensor Circuit | ECM | DTC P0110 or P0111
P0111 | Intake Air Temperature (IAT) Sensor Performance | ECM | DTC P0110 or P0111
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM |

• | DTC P0112 or P0113 for the 1.2L engine

• | DTC P0112 or P0113 for the 1.4L DOHC engine

• | DTC P0112 or P0113 for the 1.4L SOHC engine

• | DTC P0112 or P0113 for the 1.5L engine

• | DTC P0112 or P0113 for the 1.6L engine

P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM |

• | DTC P0112 or P0113 for the 1.2L engine

• | DTC P0112 or P0113 for the 1.4L DOHC engine

• | DTC P0112 or P0113 for the 1.4L SOHC engine

• | DTC P0112 or P0113 for the 1.5L engine

• | DTC P0112 or P0113 for the 1.6L engine

P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM |

• | DTC P0117 or P0118 for the 1.2L engine

• | DTC P0117 or P0118 for the 1.4L DOHC engine

• | DTC P0117 or P0118 for the 1.4L SOHC engine

• | DTC P0117 or P0118 for the 1.5L engine

• | DTC P0117 or P0118 for the 1.6L engine

P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM |

• | DTC P0117 or P0118 for the 1.2L engine

• | DTC P0117 or P0118 for the 1.4L DOHC engine

• | DTC P0117 or P0118 for the 1.4L SOHC engine

• | DTC P0117 or P0118 for the 1.6L engine

P0118 | -- | ECM | DTC P0117 or P0118
P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine

• | DTC P0122 or P0123 for the 1.4L DOHC engine

• | DTC P0122 or P0123 for the 1.4L SOHC engine

• | DTC P0122 or P0123 for the 1.5L engine

P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135
P0123 | Throttle Position (TP) Sensor Circuit High Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine

• | DTC P0122 or P0123 for the 1.4L DOHC engine

• | DTC P0122 or P0123 for the 1.4L SOHC engine

• | DTC P0122 or P0123 for the 1.5L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6L engine

P0125 | Engine Coolant Temperature (ECT) Insufficient for Close Loop | ECM | DTC P0125 or P0128
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM |

• | DTC P0131 or P0137 for the 1.2L engine

• | DTC P0131 or P0132 for the 1.4L DOHC engine

• | DTC P0131 or P0132 for the 1.4L SOHC engine

• | DTC P0131 or P0132 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine

P0132 | HO2S Circuit High Voltage Sensor 1 | ECM |

• | DTC P0132 or P0138 for the 1.2L engine

• | DTC P0131 or P0132 for the 1.4L DOHC engine

• | DTC P0131 or P0132 for the 1.4L SOHC engine

• | DTC P0131 or P0132 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine

P0133 | HO2S Slow Response Sensor 1 | ECM |

• | DTC P0133 for the 1.2L engine

• | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine

• | DTC P0133, P1133, or P1134 for the 1.4L SOHC engine

• | DTC P0133 or P0139 for the 1.6L engine

P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM |

• | DTC P0134 or P0140 for the 1.4L DOHC engine

• | DTC P0134 or P0140 for the 1.4L SOHC engine

• | DTC P0134 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine

P0135 | HO2S Heater Performance Sensor 1 | ECM |

• | DTC P0135 or P0141 for the 1.2L engine

• | DTC P0135 or P0141 for the 1.4L DOHC engine

• | DTC P0135 or P0141 for the 1.4L SOHC engine

• | DTC P0135 or P0141 for the 1.6L engine

P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM |

• | DTC P0131 or P0137 for the 1.2L engine

• | DTC P0137 or P0138 for the 1.4L DOHC engine

• | DTC P0137 or P0138 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine

P0138 | HO2S Circuit High Voltage Sensor 2 | ECM |

• | DTC P0132 or P0138 for the 1.2L engine

• | DTC P0137 or P0138 for the 1.4L DOHC engine

• | DTC P0137 or P0138 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine

P0139 | HO2S Slow Response Sensor 2 | ECM | DTC P0133 or P0139
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM |

• | DTC P0140 for the 1.2L engine

• | DTC P0134 or P0140 for the 1.4L DOHC engine

• | DTC P0134 or P0140 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine

P0141 | HO2S Heater Performance Sensor 2 | ECM |

• | DTC P0135 or P0141 for the 1.2L engine

• | DTC P0135 or P0141 for the 1.4L DOHC engine

• | DTC P0135 or P0141 for the 1.4L SOHC engine

• | DTC P0135 or P0141 for the 1.6L engine

P0171 | Fuel Trim System Lean | ECM |

• | DTC P0171 or P0172 for the 1.2L engine

• | DTC P0171 or P0172 for the 1.4L DOHC engine

• | DTC P0171 or P0172 for the 1.4L SOHC engine

• | DTC P0171, P0172, P2187, or P2188 for the 1.6L engine

P0172 | Fuel Trim System Rich | ECM |

• | DTC P0171 or P0172 for the 1.2L engine

• | DTC P0171 or P0172 for the 1.4L DOHC engine

• | DTC P0171 or P0172 for the 1.4L SOHC engine

• | DTC P0171, P0172, P2187, or P2188 for the 1.6L engine

P0201 | Injector 1 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4 SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0202 | Injector 2 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0203 | Injector 3 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0204 | Injector 4 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0217 | Engine Coolant Over Temperature | ECM | DTC P0217
P0222 | Idle Speed Control (ISP) Motor Position Sensor Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135
P0223 | Idle Speed Control (ISP) Motor Position Sensor Circuit High Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
P0300 | Engine Misfire Detected | ECM |

• | DTC P0300 for the 1.2L engine

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine

P0301 | Cylinder 1 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine

P0302 | Cylinder 2 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine

P0303 | Cylinder 3 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine

P0304 | Cylinder 4 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine

P0315 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P0315
P0317 | Rough Road Sensing System Input Not Present | ECM | DTC P0317 for the 1.4L DOHC engine or DTC P0317 for the 1.4L SOHC engine
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324 for the 1.4L DOHC engine or DTC P0324 for the 1.6L engine
P0325 | Knock Sensor (KS) Circuit | ECM |

• | DTC P0325 for the 1.4L DOHC engine

• | DTC P0325 for the 1.4L SOHC engine

• | DTC P0325 for the 1.5L engine

• | DTC P0325 for the 1.6L engine

P0327 | Knock Sensor (KS) Circuit | ECM | DTC P0327 for the 1.2L engine or DTC P0327 for the 1.5L engine
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0335, P0336, or P0337 for the 1.4L DOHC engine

• | DTC P0335 or P0336 for the 1.6L engine

P0336 | Crankshaft Position (CKP) Sensor Performance | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0335, P0336, or P0337 for the 1.4L DOHC engine

• | DTC P0336 or P0337 for the 1.4L SOHC engine

• | DTC P0336 or P0337 for the 1.5L engine

• | DTC P0335 or P0336 for the 1.6L engine

P0337 | Crankshaft Position (CKP) Sensor Circuit Low Duty Cycle | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0336 or P0337 for the 1.4L SOHC engine

• | DTC P0336 or P0337 for the 1.5L engine

P0340 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016 or P0340
P0341 | Camshaft Position (CMP) Sensor Performance | ECM |

• | DTC P0341 or P0342 for the 1.2L engine

• | DTC P0341 or P0342 for the 1.4L SOHC engine

• | DTC P0341 or P0342 for the 1.5L engine

P0342 | Camshaft Position (CMP) Sensor Circuit Low Voltage | ECM |

• | DTC P0341 or P0342 for the 1.2L engine

• | DTC P0341 or P0342 for the 1.4L SOHC engine

• | DTC P0341 or P0342 for the 1.5L engine

P0351 | Ignition Coil 1 and 4 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.2L engine

• | DTC P0351 or P0352 for the 1.4L DOHC engine

• | DTC P0351 or P0352 for the 1.4L SOHC engine

• | DTC P0351 or P0352 for the 1.5L engine

• | DTC P0351 or P0352 for the 1.6L engine

P0352 | Ignition Coil 2 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.2L engine

• | DTC P0351 or P0352 for the 1.4L DOHC engine

• | DTC P0351 or P0352 for the 1.4L SOHC engine

• | DTC P0351 or P0352 for the 1.5L engine

• | DTC P0351 or P0352 for the 1.6L engine

P0400 | Exhaust Gas Recirculation (EGR) Flow Incorrect | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine

P0401 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine

P0402 | Exhaust Gas Recirculation (EGR) Flow Excessive | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine

P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404
P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L engine

P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L engine

P0406 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit High Voltage | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L engine

P0420 | Catalyst System Low Efficiency | ECM |

• | DTC P0420 for the 1.2L engine

• | DTC P0420 for the 1.4L DOHC engine

• | DTC P0420 for the 1.4L SOHC engine

• | DTC P0420 for the 1.6L engine

P042E | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine or DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L engine
P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM | DTC P0442 or P0456
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM |

• | DTC P0443 for the 1.4L DOHC engine

• | DTC P0443 for the 1.4L SOHC engine

• | DTC P0443 for the 1.5L engine

P0444 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0444 or P0445
P0445 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0444 or P0445
P0446 | Evaporative Emission (EVAP) Vent System Performance | ECM | DTC P0446
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451 or P0454
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0452 or P0453
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0452 or P0453
P0454 | Fuel Tank Pressure (FTP) Sensor Intermittent | ECM | DTC P0451 or P0454
P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM | DTC P0455
P0456 | Evaporative Emission (EVAP) System Very Small Leak Detected | ECM | DTC P0442 or P0456
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Open | ECM | DTC P0458 or P0459
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0458 or P0459
P0461 | Fuel Level Sensor Circuit Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0463
P0464 | Fuel Level Circuit Intermittent | ECM | DTC P0464
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480 or P0481
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480 or P0481
P0496 | Evaporative Emission (EVAP) System Continuous Purge Flow | ECM | DTC P0496
P0498 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Open | ECM | DTC P0498 or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Shorted | ECM | DTC P0498 or P0499
P0501 | Vehicle Speed Sensor (VSS) Circuit | ECM | DTC P0501
P0502 | Vehicle Speed Sensor (VSS) Circuit | ECM |

• | DTC P0502 for the 1.4L DOHC engine

• | DTC P0502 for the 1.4L SOHC engine

• | DTC P0502 for the 1.5L engine

• | DTC P0502 for the 1.6L engine

P0506 | Idle Speed Low | ECM |

• | DTC P0506 or P0507 for the 1.4L DOHC engine

• | DTC P0506 or P0507 for the 1.4L SOHC engine

• | DTC P0506 or P0507 for the 1.6L engine

P0507 | Idle Speed High | ECM |

• | DTC P0506 or P0507 for the 1.4L DOHC engine

• | DTC P0506 or P0507 for the 1.4L SOHC engine

• | DTC P0506 or P0507 for the 1.6L engine

P0510 | Idle Position Switch Circuit | ECM | DTC P0510
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0562 | System Voltage Low | ECM, TCM | DTC P0562 or DTC P0562
P0563 | System Voltage High | ECM, TCM | DTC P0563 or DTC P0563
P0564 | Cruise Control Multi-function Switch Circuit | ECM | DTC P0564
P0565 | Cruise Control Switch Circuit | ECM | DTC P0565
P0567 | Cruise Control Resume Switch Circuit | ECM | DTC P0567
P0568 | Cruise Control Set Switch Circuit | ECM | DTC P0568
P0571 | Cruise Control Brake Switch 1 Circuit | ECM | DTC P0571
P0600 | Control Module Internal Performance | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P0601 | Control Module Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

P0601 | Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601 or P1790
P0602 | Control Module Not Programmed | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

P0603 | Control Module Long Term Memory Reset | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

P0604 | Control Module Random Access Memory (RAM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

P0604 | Control Module Random Access Memory (RAM) | TCM | DTC P0604
P0605 | Control Module Programming Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

P0606 | Control Module Internal Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

P0607 | Control Module Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

P061B | Control Module Internal Performance | ECM | DTC P061B or P161B
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0628 or P0629
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641 or P0651
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650 or P1650 for the 1.2L engine or DTC P0650 for the 1.6L engine
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641 or P0651
P0656 | Fuel Level Output Circuit | ECM | DTC P0656
P0660 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit | ECM | DTC P0660 for the 1.4L DOHC engine or DTC P0660 for the 1.6L engine
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM |

• | DTC P0700 for the 1.4L DOHC engine

• | DTC P0700 for the 1.4L SOHC engine

• | DTC P0700 for the 1.6L engine

P0705 | Transmission Range Sensor Circuit | TCM | DTC P0705
P0706 | Transmission Range (TR) Switch Performance | TCM | DTC P0706
P0711 | Transmission Fluid Temperature Sensor (TFT) Sensor Performance | TCM | DTC P0711
P0712 | Transmission Fluid Temperature Sensor Low Input | TCM | DTC P0712
P0713 | Transmission Fluid Temperature Sensor Circuit High input | TCM | DTC P0713
P0717 | Input Speed Sensor - No Signal | TCM | DTC P0717
P0722 | Output Speed Sensor Circuit No Signal | TCM | DTC P0722
P0727 | Engine Speed Signal Circuit | TCM | DTC P0727
P0741 | Torque Converter Clutch (TCC) System-Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch Circuit Stuck On | TCM | DTC P0742
P0743 | Torque Converter Clutch Circuit Electrical | TCM | DTC P0743
P0748 | Pressure Control Solenoid Electrical | TCM | DTC P0748
P0751 | Shift Solenoid 1 Performance or Stuck Off | TCM | DTC P0751
P0752 | Shift Solenoid 1 Performance Stuck On | TCM | DTC P0752
P0753 | Shift Solenoid 1 Electrical | TCM | DTC P0753
P0756 | Shift Solenoid 2 Performance or Stuck Off | TCM | DTC P0756
P0757 | Shift Solenoid (SS) 2 Performance Stuck On | TCM | DTC P0757
P0758 | Shift Solenoid 2 Electrical | TCM | DTC P0758
P0785 | Shift Timing Solenoid | TCM | DTC P0785 or P1710
P0787 | Shift Timing Solenoid Low Voltage | TCM | DTC P0787
P0788 | Shift Timing Solenoid High Voltage | ECM | DTC P0788
P0834 | Clutch Pedal Switch Circuit Low Voltage | ECM | DTC P0834
P0835 | Clutch Pedal Switch Circuit High Voltage | ECM | DTC P0835
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0963
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0974
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0976
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0977
P1106 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1106 or P1107 for the 1.4L DOHC engine

• | DTC P1106 or P1107 for the 1.4L SOHC engine

• | DTC P1106 or P1107 for the 1.5L engine

P1107 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1106 or P1107 for the 1.4L DOHC engine

• | DTC P1106 or P1107 for the 1.4L SOHC engine

• | DTC P1106 or P1107 for the 1.5L engine

P1111 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1111 or P1112 for the 1.4L DOHC engine

• | DTC P1111 or P1112 for the 1.4L SOHC engine

• | DTC P1111 or P1112 for the 1.5L engine

P1112 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1111 or P1112 for the 1.4L DOHC engine

• | DTC P1111 or P1112 for the 1.4L SOHC engine

• | DTC P1111 or P1112 for the 1.5L engine

P1114 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1114 or P1115 for the 1.4L DOHC engine

• | DTC P1114 or P1115 for the 1.4L SOHC engine

• | DTC P1114 or P1115 for the 1.5L engine

P1115 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1114 or P1115 for the 1.4L DOHC engine

• | DTC P1114 or P1115 for the 1.4L SOHC engine

• | DTC P1114 or P1115 for the 1.5L engine

P1121 | Throttle Position (TP) Sensor Circuit Intermittent High Voltage | P1121 |

• | DTC P1121 or P1122 for the 1.4L DOHC engine

• | DTC P1121 or P1122 for the 1.4L SOHC engine

• | DTC P1121 or P1122 for the 1.5L engine

P1122 | Throttle Position (TP) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1121 or P1122 for the 1.4L DOHC engine

• | DTC P1121 or P1122 for the 1.4L SOHC engine

• | DTC P1121 or P1122 for the 1.5L engine

P1133 | HO2S Insufficient Switching Sensor 1 | ECM | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine or DTC P0133, P1133, or P1134 for the 1.4L SOHC engine
P1134 | HO2S Transition Time Ratio Sensor 1 | ECM | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine or DTC P0133, P1133, or P1134 for the 1.4L SOHC engine
P1137 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1137 or P1166
P1138 | HO2S Circuit High Voltage During Diesel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1138 or P2297
P1166 | HO2S Circuit Low Voltage During Power Enrichment Sensor 2 | ECM | DTC P1166 for the 1.4L DOHC engine or DTC P1137 or P1166 for the 1.6L engine
P1167 | HO2S Circuit High Voltage During Diesel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1167 for the 1.4L DOHC engine or DTC P1167 for the 1.4L SOHC engine
P1171 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1171 for the 1.4L DOHC engine or DTC P1171 for the 1.4L SOHC engine
P1230 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P1230 or P1231
P1231 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P1230 or P1231
P1320 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1320
P1321 | Crankshaft Position (CKP) Reluctor Wheel Performance | ECM | DTC P1321
P1336 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1336 for the 1.4L DOHC engine or DTC P1336 for the 1.4L SOHC engine
P1380 | Misfire Detected - Rough Road Data Not Available | ECM | DTC P1380 or P1381
P1381 | Misfire Detected - No Communication With Brake Control Module | ECM | DTC P1380 or P1381 for the 1.4L DOHC engine or DTC P1380 or P1381 for the 1.4L SOHC engine
P1382 | Wheel Speed Sensor Circuit Performance | ECM | DTC P1382 or P1385
P1385 | Wheel Speed Sensor Circuit | ECM | DTC P1382 or P1385
P1390 | Left Driven Wheel Speed Sensor Circuit | ECM | DTC P1390 or P1396
P1391 | Rough Road Sensor Performance | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L engine

P1392 | Rough Road Sensor Circuit Low Voltage | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L engine

P1393 | Rough Road Sensor Circuit High Voltage | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L engine

P1396 | Wheel Speed Sensor Circuit w/o ABS | ECM |

• | DTC P1390 or P1396 for the 1.2L engine

• | DTC P1396 or P1397 for the 1.4L DOHC engine

• | DTC P1396 or P1397 for the 1.6L engine

P1397 | Wheel Speed Sensor Circuit w/ABS | ECM | DTC P1396 or P1397 for the 1.4L DOHC engine or DTC P1396 or P1397 for the 1.6L engine
P1402 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine

P1403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404
P1404 | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

P1504 | Vehicle Speed Output Circuit 2 | ECM | DTC P1504
P1511 | Idle Speed Control (ISC) Motor Control Circuit | ECM | DTC P1511, P1512, or P1513
P1512 | Idle Speed Control (ISC) System | ECM | DTC P1511, P1512, or P1513
P1513 | Idle Speed Control (ISC) System Performance | ECM | DTC P1511, P1512, or P1513
P1516 | Throttle Actuator control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119
P1601 | Lost Communication with TCM | ECM |

• | DTC P1601 for the 1.4L DOHC engine

• | DTC P1601 for the 1.4L SOHC engine

• | DTC P1601 for the 1.5L engine

P1607 | -- | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P1610 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P1610 or P1611
P1611 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P1610 or P1611
P161B | Control Module Torque Performance | ECM | DTC P061B or P161B
P1626 | Lost Communication with Theft Deterrent Control Module | TDM | DTC P1626
P1650 | Malfunction Indicator Lamp (MIL) Control Circuit High Voltage | ECM | DTC P1650 or P1651
P1650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P1651 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM | DTC P1650 or P1651
P1660 | Malfunction Indicator Lamp (MIL) Control Circuit High Voltage | ECM | DTC P1660 or P1661
P1661 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM | DTC P1660 or P1661
P1701 | Engine Coolant Temperature (ECT) Sensor Circuit | TCM | DTC P1701 or P1792
P1702 | Engine Torque Signal Error | TCM | DTC P1702
P1710 | Timing Solenoid Electrical | TCM | DTC P0785 or P1710
P1781 | Engine Torque Signal Error | TCM | DTC P1781
P1790 | Internal Control Module Memory Checksum Error | TCM | DTC P0601 or P1790
P1791 | Throttle Position (TP) Sensor Circuit | TCM | DTC P1791
P1792 | Engine Coolant Signal | TCM | DTC P1701 or P1792
P2076 | Intake Manifold Tuning (IMT) Valve Position Sensor Performance | ECM | DTC P2076, P2077, or P2078
P2077 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit Low Voltage | ECM | DTC P2076, P2077, or P2078
P2078 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit High Voltage | ECM | DTC P2076, P2077, or P2078
P2101 | Idle Speed Control (ISC) Motor Control Circuit | ECM | DTC P2101, P2118, or P2119
P2101 | Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119
P2104 | Throttle Actuator Control (TAC) System - Forced Engine Idle | ECM | DTC P2104, P2105, P2106, or P2110
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2104, P2105, P2106, or P2110
P2106 | Throttle Control System Performance - Throttle Limitation Active | ECM | DTC P2104, P2105, P2106, or P2110
P2110 | Throttle Actuator Control (TAC) System - Forced Limited Engine Speed | ECM | DTC P2104, P2105, P2106, or P2110
P2118 | Idle Speed Control (ISC) System | ECM | DTC P2101, P2118, or P2119
P2119 | Idle Speed Control (ISC) System Performance | ECM | DTC P2101, P2118, or P2119
P2119 | Throttle Closed Position Performance | ECM | DTC P1516, P2101, or P2119
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2135 | Throttle Position (TP) Sensor 1-2 Correlation | ECM | DTC P0122, P0123, P0222, P0223, or P2135
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2187 | Fuel Trim System Lean at Idle | ECM | DTC P0171, P0172, P2187, or P2188
P2188 | Fuel Trim System Rich at Idle | ECM | DTC P0171, P0172, P2187, or P2188
P2282 | Intake Manifold Air Leak | ECM | DTC P2282
P2297 | HO2S Circuit High Voltage during Diesel Fuel Cut-Off (DFCO) Sensor 2 | ECM | DTC P2297 for the 1.4L DOHC engine or DTC P1138 or P2297 for the 1.6L engine
P2610 | Control Module Ignition Off Timer Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

P2769 | Torque Converter Clutch (TCC) Control Circuit Low Voltage | TCM | DTC P2769
P2770 | Torque Converter Clutch (TCC) Control Circuit High Voltage | TCM | DTC P2770
U0101 | Lost Communication with Transmission Control Module (TCM) | TCM | DTC U0100-U0299
U0401 | Invalid Data Received from ECM/PCM | TCM | DTC U0401
U2105 | CAN Bus Error | TCM | DTC U2105