For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the lower steering column cover panel screws.
3. Turn the steering wheel in order to access the upper steering column cover panel screws. Remove the upper steering column cover panel screws.
4. Remove the upper and the lower steering column cover panels.
5. Remove the turn signal switch by pushing in on the tabs on either side of the switch housing.
6. Disconnect the electrical connectors from the turn signal switch.

### Installation Procedure

1. Connect the electrical connectors to the turn signal switch.
2. Install the turn signal switch into the switch housing.
3. Install the upper and the lower steering column cover panels.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the lower steering column cover panel screws.

Tighten
Tighten the lower steering column cover panel screws to 3 N·m (27 lb in).

5. Turn the steering wheel in order to access the upper steering column cover panel screw holes. Install the upper steering column cover panel screws.

Tighten
Tighten the upper steering column cover panel screws to 3 N·m (27 lb in).

6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .