For 1990-2009 cars

### Removal Procedure

Warning: Refer to Electric Coolant Fan Warning in the Preface section.

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the cooling fan electrical connector(s).
3. Remove the electric cooling fan mounting bolts.
4. Remove the electric cooling fan.

### Installation Procedure

Warning: If a fan blade is bent or damaged in any way, do not repair or reuse the damaged part. Always replace a bent or damaged fan blade. Fan blades that have been damaged can not be assured of proper balance and could fail and fly apart during subsequent use. This creates an extremely dangerous situation.

The fan blades must remain in proper balance. You cannot assure fan blade balance once a fan blade has been bent or damaged. A fan blade that is not in proper balance could fail and fly apart during use, creating an extremely dangerous situation.
1. Install the electric cooling fan.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the electric cooling fan mounting bolts and tighten to 4 N·m (35 lb in).
3. Connect the cooling fan electrical connector.