For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the door seal trim. Refer to Door Water Deflector Replacement .
3. Remove the outside channel molding. Refer to Front Side Door Window Channel Replacement .
4. Remove the screws that secure the glass to the window regulator.
5. Remove the bolts and the guide rail.
6. Remove the glass from the door.

### Installation Procedure

1. Install the glass in the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the guide rail and the bolts.

Tighten
Tighten the guide rail bolts to 7 N·m (62 lb in).

3. Install the glass to the window regulator with the screws.

Tighten
Tighten the door glass screws to 7 N·m (62 lb in).

4. Install the outside channel molding. Refer to Front Side Door Window Channel Replacement .
5. Install the door seal trim. Refer to Door Water Deflector Replacement .
6. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement.