For 1990-2009 cars

Connector 1: | Fuse Block - Underhood Label
Connector 2: | Fuse Block - Underhood (Bottom View)
Connector 3: | Fuse Block - Underhood X1 (LXV)
Connector 4: | Fuse Block - Underhood X1 (LDT)
Connector 5: | Fuse Block - Underhood X1 (Without LDT/LXV)
Connector 6: | Fuse Block - Underhood X2 (North America)
Connector 7: | Fuse Block - Underhood X2 (Without North America)
Connector 8: | Fuse Block - Underhood X3 (North America)
Connector 9: | Fuse Block - Underhood X3 (Without North America)
Connector 10: | Fuse Block - Underhood X4 (JM4)
Connector 11: | Fuse Block - I/P Label (Hatchback)
Connector 12: | Fuse Block - I/P Label (Notchback)
Connector 13: | Fuse Block - I/P (Bottom View)
Connector 14: | Fuse Block - I/P X1
Connector 15: | Fuse Block - I/P X2
Connector 16: | Fuse Block - I/P X3

### Fuse Block - Underhood Label

#### Fuse Block - Underhood Label Usage

No. | Fuse | Rating | Description
--- | --- | --- | ---
Ef1 | BATT Fuse | 50A | Fuse Block - I/P F7, F10, F11, F12, F13, F14, F15, F16, F18, F21 Fuses
Ef2 | P/WINDOW1 Fuse | 30A | Window Switch - Driver
Ef3 | IGN2/ST Fuse | 30A | Ignition Switch
Ef4 | ACC/IGN1 Fuse | 30A | Ignition Switch
Ef5 | ABS Fuse | 50A | Electronic Brake Control Module (EBCM)
Ef6 | FAN HI Fuse | 30A | FAN HI Relay
Ef7 | P/WINDOW2 Fuse | 10A | Window Switch - Driver
Ef8 | PK/LP LH Fuse | 10A | License Lamp, Position Lamp/Headlamp Leveling Actuator - Left, Tail Lamp - Left
Ef9 | PK/LP RH Fuse | 10A | Fuse Block - I/P PARK Relay (T61), JX202, Position Lamp/Headlamp Leveling Actuator - Right, Tail Lamp - Right
Ef10 | Empty | -- | Not Used
Ef11 | FUEL PUMP Fuse | 15A | FUEL PUMP Relay
Ef12 | ECU Fuse | 10A | Engine Control Module (ECM), Transmission Control Module (TCM) (MLQ)
Ef13 | EMS1 Fuse | 15A | A/C Relay, Engine Control Module (ECM), FAN HI Relay, FAN LOW Relay, Fuel Injector 1, Fuel Injector 2, Fuel Injector 3, Fuel Injector 4, Ignition Coil Module
Ef14 | EMS2 Fuse | 15A | Camshaft Position (CMP) Sensor, Evaporative Emission (EVAP) Canister Purge Solenoid Valve, Exhaust Gas Recirculation (EGR) Valve, Heated Oxygen Sensor (HO2S) 1, Heated Oxygen Sensor (HO2S) 2, Port Deactivation (PDA) Solenoid (1.2L)
Ef15 | HAZARD Fuse | 15A | Hazard Switch and Hood Ajar Switch
Ef16 | Empty | -- | Not Used
Ef17 | SPARE Fuse | 20A | Not Used
Ef18 | SPARE Fuse | 15A | Not Used
Ef19 | SPARE Fuse | 10A | Not Used
Ef20 | H/L LOW RH Fuse | 10A | Headlamp - Right
Ef21 | H/L LOW LH Fuse | 10A | Headlamp - Left, and Headlamp Leveling Switch
Ef22 | FRT FOG Fuse | 15A | FRT FOG Relay
Ef23 | H/L HI Fuse | 15A | H/L HI Relay
Ef24 | FAN LOW Fuse | 20A | FAN LOW Relay
Ef25 | A/C COMP Fuse | 10A | A/C Relay
-- | A/C Relay | -- | A/C Compressor Clutch, and Engine Control Module (ECM)
-- | FAN HI Relay | -- | Cooling Fan, Cooling Fan Resistor, and Engine Control Module (ECM)
-- | FAN LOW Relay | -- | Cooling Fan Resistor, and Engine Control Module (ECM)
-- | FRT FOG Relay | -- | Fog Lamp - Left Front, Fog Lamp - Right Front, Fuse Block - I/P, and Instrument Panel Cluster (IPC)
-- | FUEL PUMP Relay | -- | Engine Control Module (ECM), and Fuel Pump and Sender Assembly
-- | H/L HI Relay | -- | Headlamp - Left, Headlamp - Right, Headlamp Switch, Instrument Panel Cluster (IPC)
-- | H/L LOW Relay | -- | Fuse Block - I/P, Fuse Block - Underhood EF20 and EF21 Fuses
-- | MAIN Relay | -- | Engine Control Module (ECM), Fuse Block - Underhood EF13 and EF14 Fuses
-- | PARK LAMP Relay | -- | Fuse Block - I/P, Fuse Block - Underhood EF8 and EF9 Fuses
-- | P/WINDOW Relay | -- | Fuse Block - I/P, Fuse Block - Underhood EF2 and EF7 Fuses

### Fuse Block - Underhood (Bottom View)

### Fuse Block - Underhood X1 (LXV)

#### Connector Part Information

- OEM: 0-936352-1
- Service: N/A
- Description: 40-Way F 090 SPT Hybrid Series (GY)

#### Fuse Block - Underhood X1 (LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | 67 | A/C Compressor Clutch Coil Supply Voltage
2 | OG/BK | 1732 | 5-Volt Reference
3 | OG/BK | 1732 | 5-Volt Reference
4 | -- | -- | Not Used
5 | RD/WH | -- | Battery Positive Voltage
6 | -- | -- | Not Used
7 | OG/BK | 1732 | 5-Volt Reference
OG/BK | 1732 | 5-Volt Reference
8 | -- | -- | Not Used
9 | OG/BK | 812 | AC Compressor Relay
10 | -- | -- | Not Used
11 | PK | 539 | Ignition 1 Voltage
12 | -- | -- | Not Used
13 | BN | 415 | Engine Coolant Temperature Sensor 2 Signal
14 | -- | -- | Not Used
15 | WH | 1977 | Rear Fog Lamp Relay Control
16 | OG/BK | 441 | Main Relay Control
17-19 | -- | -- | Not Used
20 | PK | 539 | Ignition 1 Voltage
21 | D-BU | 473 | High Speed Cooling Fan Relay Control
22 | OG | 1733 | 5-Volt Reference
23 | OG | 1733 | 5-Volt Reference
24 | OG | 1733 | 5-Volt Reference
25 | -- | -- | Not Used
26 | RD/WH | 440 | Battery Positive Voltage
27-28 | -- | -- | Not Used
29 | L-GN | 497 | Fuel Pump Relay Control
30 | D-GN | 355 | Driver Door Lock Relay Lock Control
31 | BN | 413 | Heated Oxygen Sensor Low Signal
32 | PU | 1670 | Heated Oxygen Sensor High Signal Bank 2 Sensor (2)
33 | OG | 1733 | 5-Volt Reference
34 | OG | 1733 | 5-Volt Reference
35 | -- | -- | Not Used
36 | YE | 5 | Crank Voltage
37 | BN | 1671 | Heated Oxygen Sensor Low Signal Bank 2 Sensor (2)
38 | BN | 323 | Starter Relay Controls
39-40 | -- | -- | Not Used

### Fuse Block - Underhood X1 (LDT)

#### Connector Part Information

- OEM: 1-936321-2
- Service: N/A
- Description: 32-Way F 090 SPT Hybrid Series (BK)

#### Fuse Block - Underhood X1 (LDT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 415 | Engine Coolant Temperature Sensor 2 Signal
2 | OG | 1733 | 5-Volt Reference
3 | RD/WH | 440 | Battery Positive Voltage
4 | L-BU | 1031 | Ignition Timing Stepper Motor Coil 1 High
L-BU | 1031 | Ignition Timing Stepper Motor Coil 1 High
5 | OG | 1733 | 5-Volt Reference
OG | 1733 | 5-Volt Reference
6 | L-BU | 834 | Vehicle Speed Signal
L-BU | 830 | Wheel Speed Sensor Signal Left Front
7 | OG/BK | 1732 | 5-Volt Reference
8 | BN | 413 | Heated Oxygen Sensor High Signal
9 | WH | 1977 | Rear Fog Lamp Relay Control
10 | -- | -- | Not Used
11 | BK | 51 | Ground
12 | OG | 1733 | 5-Volt Reference
OG | 1733 | 5-Volt Reference
13 | L-BU | 1031 | 5-Volt Reference
14 | YE | 873 | Left Front Wheel Speed Sensor Low Reference
15 | PU/WH | 67 | A/C Compressor Clutch Coil Supply Voltage
16 | BN | 1671 | Heated Oxygen Sensor Low Signal Bank 2 Sensor (2)
17 | -- | -- | Not Used
18 | OG | 1733 | 5-Volt Reference
19 | BN | 808 | Low Reference
20 | OG/BK | 1732 | 5-Volt Reference
OG/BK | 1732 | 5-Volt Reference
21 | OG/BK | 1732 | 5-Volt Reference
OG/BK | 1732 | 5-Volt Reference
22 | OG/BK | 812 | 5-Volt Reference
23 | L-GN | 497 | Fuel Pump Relay Control
24 | -- | -- | Not Used
25 | BN | 808 | Low Reference
26 | BN | 808 | Low Reference
BN | 808 | Low Reference
27 | PK | 539 | Ignition 1 Voltage
28 | PK | 539 | Ignition 1 Voltage
29 | PK | 539 | Ignition 1 Voltage
30 | OG/BK | 441 | Main Relay Control
31 | D-BU | 473 | High Speed Cooling Fan Relay Control
32 | D-GN | 355 | Low Speed Cooling Fan Relay Control

### Fuse Block - Underhood X1 (Without LDT/LXV)

#### Connector Part Information

- OEM: 1-936321-2
- Service: N/A
- Description: 32-Way F 090 SPT Hybrid Series (BK)

#### Fuse Block - Underhood X1 (Without LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 732 | A/C Refrigerant High Temperature Sensor Signal (1.2L)
2 | OG | 1733 | 5-Volt Reference
3 | RD/WH | 440 | Battery Positive Voltage
RD/WH | 440 | Battery Positive Voltage (L95/LXT/LV8)
4 | GY | 1031 | Ignition Timing Stepper Motor Coil 1 High (1.2L+NQU)
L-BU | 1031 | Ignition Timing Stepper Motor Coil 1 High (1.4L/1.6L)
L-BU | 1937 | Low Reference (1.5L)
L-BU | 1937 | Low Reference (1.5L)
5 | OG | 1733 | 5-Volt Reference (1.2L)
OG | 1733 | 5-Volt Reference (1.2L)
PK | 539 | Ignition 1 Voltage (1.4L/1.5L/1.6L)
PK | 539 | Ignition 1 Voltage (1.4L/1.5L/1.6L)
6 | BN | 834 | Vehicle Speed Signal (1.4L/1.6L)
L-BU | 830 | Wheel Speed Sensor Signal Left Front (1.2L)
7 | PK/BK | 1739 | Ignition 1 Voltage (1.4L/1.6L)
PK/BK | 1739 | Ignition 1 Voltage (1.4L/1.6L)
OG/BK | 1732 | 5-Volt Reference (1.2L)
OG/BK | 1732 | 5-Volt Reference (1.2L)
8 | BN | 413 | Heated Oxygen Sensor High Signal (1.4L/1.6L)
9 | PU | 1670 | Heated Oxygen Sensor Low Signal Bank 2 Sensor (2) (1.4L/1.6L)
10 | L-BU | 733 | Air Temperature Door Position Signal (1.2L)
11 | PK | 539 | Ignition 1 Voltage (1.2L/1.5L)
BK | 50 | Ground (1.4L/1.6L)
12 | PK | 539 | Ignition 1 Voltage (1.4L/1.5L/1.6L)
PK | 539 | Ignition 1 Voltage (1.4L/1.5L/1.6L)
OG | 1733 | 5-Volt Reference (1.2L)
OG | 1733 | 5-Volt Reference (1.2L)
13 | GY | 1031 | 5-Volt Reference (1.2L)
GY | 1031 | 5-Volt Reference (1.2L)
L-BU | 1031 | 5-Volt Reference (1.4L/1.6L)
L-BU | 1031 | 5-Volt Reference (1.4L/1.6L)
L-BU | 1937 | Low Reference (1.5L)
L-BU | 1937 | Low Reference (1.5L)
14 | YE | 873 | Left Front Wheel Speed Sensor Low Reference (1.2L)
15 | PU/WH | 67 | A/C Compressor Clutch Coil Supply Voltage
16 | BN | 1671 | Heated Oxygen Sensor Low Signal Bank 2 Sensor (2)
17 | -- | -- | Not Used
18 | OG | 1733 | 5-Volt Reference (1.2L)
PK | 539 | Battery Positive Voltage (1.4L/1.5L/1.6L)
19 | BN | 808 | Low Reference
BN | 808 | Low Reference (1.4L/1.5L/1.6L)
20 | OG/BK | 1732 | 5-Volt Reference (1.2L)
OG/BK | 1732 | 5-Volt Reference (1.2L)
PK | 1739 | Ignition 1 Voltage (1.5L)
PK/BK | 1739 | Ignition 1 Voltage (1.4L/1.6L)
PK/BK | 1739 | Ignition 1 Voltage (1.4L/1.6L)
21 | OG/BK | 1732 | 5-Volt Reference (1.2L)
OG/BK | 1732 | 5-Volt Reference (1.2L)
PK/BK | 1739 | Ignition 1 Voltage (1.4L/1.6L)
PK | 1739 | Ignition 1 Voltage (1.5L)
22 | OG/BK | 812 | 5-Volt Reference (1.2L)
23 | L-GN | 497 | Fuel Pump Relay Control
24 | -- | -- | Not Used
25 | BN | 808 | Low Reference (1.4L/1.5L/1.6L)
BN | 808 | Low Reference (1.4L/1.5L/1.6L)
26 | BN | 808 | Low Reference
BN | 808 | Low Reference
27 | PK | 539 | Ignition 1 Voltage
PK | 539 | Ignition 1 Voltage (1.4L/1.6L)
28 | PK | 539 | Ignition 1 Voltage
29 | PK | 539 | Ignition 1 Voltage (1.2L/1.5L)
PK | 539 | Ignition 1 Voltage
30 | OG/BK | 441 | Main Relay Control (1.2L)
31 | D-BU | 473 | High Speed Cooling Fan Relay Control
32 | D-GN | 335 | Low Speed Cooling Fan Relay Control

### Fuse Block - Underhood X2 (North America)

#### Connector Part Information

- OEM: 1-936321-2
- Service: N/A
- Description: 32-Way F 090 SPT Hybrid Series (BK)

#### Fuse Block - Underhood X2 (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 539 | Ignition 1 Voltage
2 | PK | 539 | Ignition 1 Voltage (JM4)
3 | RD/WH | -- | Ignition 1 Voltage
4 | L-GN/BK | -- | Battery Positive Voltage
5 | L-GN/BK | 580 | Left Headlamp Low Beam Supply Voltage
6 | RD/BK | 142 | Battery Positive Voltage
7 | RD/BK | -- | Battery Positive Voltage
8 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
9 | RD/WH | 440 | Battery Positive Voltage
10 | RD/WH | 440 | Battery Positive Voltage (UA5)
11 | PU | 638 | Power Window Enable Relay Control
12 | PK | -- | Ignition 1 Voltage
13 | PK | 539 | Ignition 1 Voltage
14 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
15 | BN/WH | 312 | Right Headlamp Low Beam Supply Voltage
16 | YE | 712 | Left Headlamp Low Beam Supply Voltage
17-18 | -- | -- | Not Used
19 | BN | 1671 | Heated Oxygen Sensor Low Signal Bank 2 Sensor (2)
20 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
21 | L-BU | 1346 | Headlamp Relay Control
22 | YE | 712 | Left Headlamp Low Beam Supply Voltage
23-24 | -- | -- | Not Used
25 | D-BU | 7002 | Run Relay Out
26 | RD/BK | 42 | Battery Positive Voltage
27 | L-GN/BK | 580 | Supply Voltage
28-29 | -- | -- | Not Used
30 | WH | 352 | Headlamp Relay Coil Supply Voltage
31 | PU | 1670 | Heated Oxygen Sensor High Signal Bank 2 Sensor (2)
32 | BN | 413 | Heated Oxygen Sensor Low Signal

### Fuse Block - Underhood X2 (Without North America)

#### Connector Part Information

- OEM: 2-936321-3
- Service: N/A
- Description: 32-Way F 090 SPT Hybrid Series (GY)

#### Fuse Block - Underhood X2 (Without North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
3 | -- | -- | Not Used
4 | RD/BK | 142 | Battery Positive Voltage
5 | -- | -- | Not Used
6 | PU | 709 | Left Park Lamp Supply Voltage
7 | RD/BK | 242 | Battery Positive Voltage
8 | -- | -- | Not Used
9 | BN/WH | 309 | Right Park Lamp Supply Voltage
10 | BN | 415 | Engine Coolant Temperature Sensor 2 Signal
D-BU | 732 | Evaporative Temperature Sensor Low Reference
11 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
12 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
13 | -- | -- | Not Used
14 | PU | 709 | Left Park Lamp Supply Voltage
15 | BN/WH | 309 | Right Park Lamp Supply Voltage
16 | PU | 638 | Power Window Enable Relay Control
17 | RD/WH | 440 | Battery Positive Voltage
18 | RD/WH | 440 | Battery Positive Voltage (UA5)
19-20 | -- | -- | Not Used
21 | BN/WH | 309 | Right Park Lamp Supply Voltage
22 | RD/WH | 440 | Battery Positive Voltage
23 | D-GN/WH | 1317 | Fog Lamp Relay Control
24 | YE | 1769 | Fog Lamp Relay Common
25 | YE | 1769 | Fog Lamp Relay Common (T96)
26 | RD/BK | 42 | Battery Positive Voltage
27 | WH | 1080 | Park Lamp Relay Control
28 | L-GN/BK | 580 | Power Window Relay Control
29 | BN | 1723 | ABS Solenoid Supply Voltage Rear
30 | L-GN/BK | 580 | Power Window Relay Control
31 | PK | 539 | Ignition 1 Voltage
PK | 539 | Ignition 1 Voltage (RHD)
32 | L-BU | 834 | Vehicle Speed Signal

### Fuse Block - Underhood X3 (North America)

#### Connector Part Information

- OEM: 3-936321-4
- Service: N/A
- Description: 32-Way F 090 SPT Hybrid Series (BN)

#### Fuse Block - Underhood X3 (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BN | 415 | Engine Coolant Temperature Sensor 2 Signal
3 | WH | 1977 | Rear Fog Lamp Relay Control
4 | -- | -- | Not Used
5 | BN | 1723 | ABS Solenoid Supply Voltage Rear
6 | BK | 50 | Ground
7 | BK | 50 | Ground
BK | 50 | Ground (T84)
8 | BK | 50 | Ground
9 | BK | 50 | Ground
10 | BK | 50 | Ground
11 | PK/BK | 1739 | Ignition 1 Voltage
12 | -- | -- | Not Used
13 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
14 | YE | 1769 | Fog Lamp Relay Common
15 | YE | 1769 | Fog Lamp Relay Common (T96)
YE | 1769 | Fog Lamp Relay Common (T96)
16 | D-GN/WH | 1317 | Fog Lamp Relay Control (T96)
17 | -- | -- | Not Used
18 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
19 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
20 | BN/WH | 309 | Right Park Lamp Supply Voltage
21 | BN/WH | 309 | Right Park Lamp Supply Voltage
BN/WH | 309 | Right Park Lamp Supply Voltage
22 | PU | 709 | Left Park Lamp Supply Voltage
23 | -- | -- | Not Used
24 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
25 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
26 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
27 | GY | 532 | Cooling Fan Motor Supply Voltage (2)
28 | L-BU | 409 | Cooling Fan Motor Supply Voltage (1)
29 | RD/WH | 440 | Battery Positive Voltage
30 | WH | 1080 | Park Lamp Relay Control
31 | BN/WH | 309 | Right Park Lamp Supply Voltage (North America)
32 | PU | 709 | Left Park Lamp Supply Voltage
PU | 709 | Left Park Lamp Supply Voltage

### Fuse Block - Underhood X3 (Without North America)

#### Connector Part Information

- OEM: 3-936321-4
- Service: N/A
- Description: 32-Way F 090 SPT Hybrid Series (BN)

#### Fuse Block - Underhood X3 (Without North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | PK | 539 | Ignition 1 Voltage
3 | PK | 539 | Ignition 1 Voltage
4 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
5 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
6 | BN/WH | 312 | Right Headlamp Low Beam Supply Voltage
7 | YE | 712 | Left Headlamp Low Beam Supply Voltage
YE | 712 | Left Headlamp Low Beam Supply Voltage
8 | PK/BK | 1739 | Ignition 1 Voltage
PK/BK | 1739 | Ignition 1 Voltage
9 | BN | 1671 | Heated Oxygen Sensor Low Signal Bank 2 Sensor (2)
10 | L-BU | 733 | Air Temperature Door Position Signal
11 | PK | 539 | Ignition 1 Voltage
12 | PK | 539 | Ignition 1 Voltage
13 | L-BU | 1346 | Headlamp Relay Control
14 | L-BU | 830 | Wheel Speed Sensor Signal Left Front
L-BU | 834 | Vehicle Speed Signal
15 | -- | -- | Not Used
16 | WH | 1977 | Rear Fog Lamp Relay Control (T9E)
PU | 1670 | Heated Oxygen Sensor High Signal Bank 2 Sensor (2) (NT3)
17 | BK | 50 | Ground
BK | 50 | Ground
18 | BK | 50 | Ground
BK | 50 | Ground
19 | BK | 50 | Ground
20 | -- | -- | Not Used
21 | YE | 873 | Left Front Wheel Speed Sensor Low Reference
22 | BN | 413 | Heated Oxygen Sensor Low Signal
23 | BK | 50 | Ground
24 | BK | 50 | Ground
BK | 50 | Ground
25 | WH | 352 | Headlamp Relay Coil Supply Voltage
26 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
27 | GY | 532 | Cooling Fan Motor Supply Voltage (2)
28 | L-BU | 409 | Cooling Fan Motor Supply Voltage (1)
29 | OG/BK | 812 | A/C Compressor Relay
30 | L-BU | 15 | Right Turn Signal Lamp Supply Voltage
31 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
32 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
D-BU | 15 | Right Turn Signal Lamp Supply Voltage

### Fuse Block - Underhood X4 (JM4)

#### Connector Part Information

- OEM: MG610557
- Service: N/A
- Description: 2-Way F 375 Series (NA)

#### Fuse Block - Underhood X4 (JM4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | 40 | Battery Positive Voltage
2 | RD | 40 | Battery Positive Voltage

### Fuse Block - I/P Label (Hatchback)

#### Fuse Block - I/P Label Usage (Hatchback)

No. | Fuse | Rating | Description
--- | --- | --- | ---
F1 | SDM Fuse | 10A | Inflatable Restraint Sensing and Diagnostic Module (SDM)
F2 | WIPER Fuse | 25A | Windshield Wiper/Washer Switch, Windshield Wiper Motor
F3 | CLUSTER Fuse | 10A | Clock, Instrument Panel Cluster (IPC), Remote Control Door Lock Receiver (RCDLR), Stop Lamp Switch
F4 | T/SIG Fuse | 10A | Hazard Switch
F5 | EMS2 Fuse | 10A | Fuse Block - Underhood, Heated Oxygen Sensor (HO2S) 2, Tank Shut-off Valve, Transmission Control Module (TCM) (MLQ), Vehicle Speed Sensor (VSS) (MFM/MLM)
F6 | EMS1 Fuse | 15A | Fuse Block - Underhood, Immobilizer
F7 | STOP LAMP Fuse | 15A | Stop Lamp Switch
F8 | CIGAR Fuse | 15A | Cigar Lighter
F9 | AUDIO Fuse | 10A | Clock, I/P Compartment Lamp Switch, Radio
F10 | OBD Fuse | 10A | Data Link Connector (DLC), Immobilizer
F11 | RR DEFOG Fuse | 25A | REAR DEFOG Relay
F12 | CLUSTER/ROOM LAMP Fuse | 10A | Dome Lamp, I/P Compartment Lamp Switch, Instrument Panel Cluster (IPC), Rear Compartment Lamp
F13 | SOCKET Fuse | 15A | Auxiliary Power Outlet
F14 | DOOR LOCK Fuse | 15A | DOOR LOCK Relay, DOOR UNLOCK Relay
F15 | RR FOG Fuse | 10A | Fuse Block - I/P Controller, REAR FOG Relay
F16 | SUN ROOF Fuse | 20A | Sunroof Control Module (CF5)
F17 | B/UP LAMP Fuse | 10A | Backup Lamp Switch, Park/Neutral Position (PNP) Switch
F18 | HORN Fuse | 15A | HORN Relay
F19 | MIRROR/SUNROOF Fuse | 10A | Dome Lamp, HVAC Control Module, Outside Rearview Mirror Switch
F20 | DEFOG MIRROR Fuse | 10A | HVAC Control Module, Outside Rearview Mirror - Driver, Outside Rearview Mirror - Passenger
F21 | AUDIO/RKE Fuse | 15A | Clock, Fuse Block - I/P, HVAC Control Module, Ignition Key Alarm Switch, Key Illumination, Outside Rearview Mirror - Driver, Outside Rearview Mirror - Passenger, Radio, Remote Control Door Lock Receiver (RCDLR)

### Fuse Block - I/P Label (Notchback)

#### Fuse Block - I/P Label Usage (Notchback)

No. | Fuse | Rating | Description
--- | --- | --- | ---
F1 | SDM Fuse | 10A | Inflatable Restraint Sensing and Diagnostic Module (SDM)
F2 | WIPER Fuse | 25A | Windshield Wiper/Washer Switch, Windshield Wiper Motor
F3 | CLUSTER Fuse | 10A | Clock, Instrument Panel Cluster (IPC), Remote Control Door Lock Receiver (RCDLR), Stop Lamp Switch
F4 | T/SIG Fuse | 10A | Hazard Switch
F5 | EMS2 Fuse | 10A | Fuse Block - Underhood, Heated Oxygen Sensor (HO2S) 2, Tank Shut-off Valve, Transmission Control Module (TCM) (MLQ), Vehicle Speed Sensor (VSS) (MFM/MLM)
F6 | EMS1 Fuse | 15A | Fuse Block - Underhood, Immobilizer
F7 | STOP LAMP Fuse | 15A | Stop Lamp Switch
F8 | CIGAR Fuse | 15A | Cigar Lighter
F9 | AUDIO/CLOCK Fuse | 10A | Clock, I/P Compartment Lamp Switch, Radio
F10 | OBD Fuse | 10A | Data Link Connector (DLC), Immobilizer
F11 | -- | -- | Not Used
F12 | CLUSTER/ROOM LAMP Fuse | 10A | Dome Lamp, I/P Compartment Lamp Switch, Instrument Panel Cluster (IPC), Rear Compartment Lamp
F13 | DEFOGGER Fuse | 25A | REAR DEFOG Relay
F14 | SUNROOF Fuse | 20A | Sunroof Control Module
F15 | RR FOG Fuse | 10A | Fuse Block - I/P Controller, REAR FOG Relay
F16 | DOOR LOCK Fuse | 15A | DOOR LOCK/UNLOCK Relay
F17 | B/UP LAMP Fuse | 10A | Backup Lamp Switch, Park/Neutral Position (PNP) Switch
F18 | HORN Fuse | 10A | HORN Relay
F19 | ELEC MIRROR Fuse | 10A | Outside Rearview Mirror Switch, HVAC Control Module, Dome Lamp
F20 | DEFOG MIRROR Fuse | 10A | HVAC Control Module, Outside Rearview Mirror - Driver, Outside Rearview Mirror - Passenger
F21 | AUDIO/RKE Fuse | 15A | Clock, Fuse Block - I/P, HVAC Control Module, Ignition Key Alarm Switch, Key Illumination, Outside Rearview Mirror - Driver, Outside Rearview Mirror - Passenger, Radio, Remote Control Door Lock Receiver (RCDLR)

### Fuse Block - I/P (Bottom View)

### Fuse Block - I/P X1

#### Connector Part Information

- OEM: 936195-1
- Service: N/A
- Description: 76-Way F 090/250 Hybrid Series (BK)

#### Fuse Block - I/P X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 641 | Ignition 2 Voltage (DL6)
BN | 641 | Ignition 2 Voltage (C37)
2 | PK | 239 | Ignition 1 Voltage
3-4 | -- | -- | Not Used
5 | D-GN/RD | 91 | Windshield Wiper Motor Relay Coil Supply Voltage
6 | -- | -- | Not Used
7 | L-BU | 74 | Park Lamp Switch Signal
L-BU | 74 | Park Lamp Switch Signal (UJ9)
8 | OG | 267 | Mirror Heater Element Voltage (DWT)
9 | BN/WH | 238 | Driver Seat Belt Switch Signal (-AJ3)
10 | RD/WH | 540 | Battery Positive Voltage
RD/WH | 540 | Battery Positive Voltage
11 | D-GN/WH | 1317 | Fog Lamp Relay Control (T96)
12 | L-BU | 20 | Stop Lamp Supply Voltage (WHB+MLQ)
13 | L-GN | 1076 | Ignition Key Cylinder Solenoid Lock Inhibit (WHB+MLQ)
14 | L-GN | 80 | Key In Ignition Switch Signal
15 | OG | 122 | Rear Fog Lamp Supply Voltage (T9E)
16 | -- | -- | Not Used
17 | BN | 641 | Ignition 3 Voltage (DL7)
18 | BN/WH | 33 | Brake Warning Indicator Control
19 | L-BU | 292 | Rear Defog Switch Signal (DWT)
20 | WH | 629 | High Beam Indicator Supply Voltage (WHB)
21 | D-GN/WH | 900 | Key Illumination Low Reference (TNK-WHB)
22 | RD/WH | 540 | Battery Positive Voltage (UY4)
RD/WH | 540 | Battery Positive Voltage (UY4)
23 | RD/WH | 540 | Battery Positive Voltage
RD/WH | 540 | Battery Positive Voltage
24 | -- | -- | Not Used
25 | YE | 112 | Windshield Wiper Switch Low/Pulse Signal
26 | WH | 193 | Rear Defogger Relay Control
27 | D-GN | 29 | Horn Control (UJ9)
D-GN | 29 | Horn Control (UA5)
28 | -- | -- | Not Used
29 | RD/BK | 242 | Battery Positive Voltage
30 | -- | -- | Not Used
31 | L-BU | 1346 | Headlamp Relay Control (LHD)
32 | YE | 1977 | Rear Fog Lamp Relay Control (T9E)
BN | 1075 | Ignition Key Cylinder Solenoid Lock Enable (WHB+MLQ)
33 | RD/WH | 540 | Battery Positive Voltage (UA5)
RD/WH | 540 | Battery Positive Voltage (-WHB)
34 | BN | 31 | Oil Pressure Indicator Control (T9E)
35 | -- | -- | Not Used
36 | OG | 300 | Ignition 3 Voltage
37 | L-GN | 1845 | Chime Control (AJ3)
38 | BN | 841 | Ignition 2 Voltage
39 | D-GN | 29 | Horn Control (AJ3)
D-GN | 29 | Horn Contro (C08)
40 | RD/WH | 240 | Battery Positive Voltage
41 | RD/WH | 240 | Battery Positive Voltage
42-44 | -- | -- | Not Used
45 | RD/WH | 1340 | Battery Positive Voltage
RD/WH | 1340 | Battery Positive Voltage (AJ3-WHB)
46 | RD/WH | 1340 | Battery Voltage - Folding Mirror (DL7)
47 | YE | 143 | Accessory Voltage
48-49 | -- | -- | Not Used
50 | WH | 156 | Courtesy Lamp Output (UA5)
51 | WH | 352 | Headlamp Relay Coil Supply Voltage
52 | -- | -- | Not Used
53 | GY/D-GN | 355 | Driver Door Lock Relay Lock Control (UA5)
54 | YE | 356 | Driver Door Lock Relay Unlock Control (UA5)
55 | PU/WH | 822 | VSS Low Signal (T44)
56 | PK | 139 | Ignition 1 Voltage
57-59 | -- | -- | Not Used
60 | YE | 43 | Accessory Voltage
61 | YE | 43 | Accessory Voltage
62 | PK | 139 | Ignition 1 Voltage (AJ3)
63 | -- | -- | Not Used
64 | PK | 639 | Ignition 1 Voltage (WHB)
PK | 639 | Ignition 1 Voltage
65 | PK | 639 | Ignition 1 Voltage
66 | RD/WH | 340 | Battery Positive Voltage
67 | -- | -- | Not Used
68 | PK | 239 | Ignition 1 Voltage (WHB+MLQ)
PK | 239 | Ignition 1 Voltage (-WHB)
69 | PK | 239 | Ignition 1 Voltage (UV8/UJ9)
PK | 1739 | Ignition 1 Voltage (WHB+AJ3)
70 | PK | 239 | Ignition 1 Voltage (UA5)
71 | BK/WH | 1352 | Dual Zone Switch Signal-Offset
72 | PK | 339 | Ignition 1 Voltage
73 | PK | 3 | Ignition Switch Output - Ignition 1
74 | BN | 4 | Accessory Voltage (-WHB)
L-GN/BK | 580 | Battery Positive Voltage (WHB)
75 | WH | 156 | Courtesy Lamp Switch Signal
76 | -- | -- | Not Used

### Fuse Block - I/P X2

#### Connector Part Information

- OEM: 368457-1
- Service: N/A
- Description: 20-Way F 090/250 Hybrid Series, Tyco (WH)

#### Fuse Block - I/P X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | GY | 295 | Door Lock Actuator Lock Control (AU3)
3 | WH | 194 | Power Door Lock Relay Feed - Unlock Coil
L-BU | 194 | Power Door Lock Relay Feed - Unlock Coil (Notchback+UA5-WHB)
4 | BK | 450 | Ground
5 | BN/WH | 33 | Brake Warning Indicator Lamp Output (LHD)
6 | WH | 156 | Courtesy Lamp Switch Signal
7 | -- | -- | Not Used
8 | RD/WH | 1340 | Battery Positive Voltage
9 | -- | -- | Not Used
10 | BN | 294 | Door Lock Actuator Unlock Control
11 | L-BU | 195 | Door Lock Control
12 | PU | 156 | Courtesy Lamp Switch Signal
PU | 156 | Courtesy Lamp Switch Signal (WHB)
13 | -- | -- | Not Used
14 | RD | 1093 | Rear Defog Element Supply Voltage
15 | RD/WH | 640 | Battery Positive Voltage
16 | YE | 143 | Accessory Voltage
17 | OG | 122 | Rear Fog Lamp Supply Voltage (T9E)
18 | GY | 157 | Interior Lamp Control
19 | -- | -- | Not Used
20 | OG | 267 | Mirror Heater Element Voltage

### Fuse Block - I/P X3

#### Connector Part Information

- OEM: 368497-1
- Service: N/A
- Description: 18-Way F 090/250 Hybrid Series, Tyco (WH)

#### Fuse Block - I/P X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used Power Window Enable Relay Control
2 | BN/WH | 33 | Brake Warning Indicator Control
BN/WH | 33 | Brake Warning Indicator Control (UY4)
3 | PK | 1739 | Ignition 1 Voltage (-WHB)
4 | -- | -- | Not Used
5 | PK | 94 | Windshield Washer Switch Signal
6 | WH | 1080 | Park Lamp Relay Control
7 | PU | 638 | Power Window Enable Relay Control (-WHB)
8 | BN | 641 | Ignition 3 Voltage
9 | PK | 539 | Ignition 1 Voltage
PK | 239 | Ignition 1 Voltage (BAH-WHB)
10 | PK | 239 | Ignition 1 Voltage (MLQ)
RD/WH | 1340 | Battery Positive Voltage (TNK)
11 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage (WHB)
12 | BN/WH | 309 | Illumination Supply Voltage
13 | L-BU | 97 | Windshield Wiper Switch Mist/Off/Low Signal
14 | BN | 96 | Windshield Wiper Switch Pulse Delay Signal
15 | WH | 352 | Headlamp Relay Coil Supply Voltage
16 | D-GN/WH | 1317 | Fog Lamp Relay Control
17 | BN/WH | 309 | Right Park Lamp Supply Voltage
18 | BN | 28 | Horn Relay Control