For 1990-2009 cars

### Removal Procedure

1. Siphon the power steering fluid from the fluid reservoir.
2. Loosen the hose clamps and remove both hoses.
3. Plug the hoses in order to prevent contaminants from entering the power steering system.
4. Remove the fluid reservoir attaching bolts and remove the fluid reservoir.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Attach the fluid reservoir with the power steering fluid reservoir attaching bolts.

Tighten
Tighten the power steering fluid reservoir attaching bolts to 7 N·m (62 lb in).

2. Connect both hoses and secure the hose clamps.

Notice: When adding fluid or making a complete fluid change, always use a power steering fluid meeting GM Spec. No. 9985010 or equivalent. Fluid for cold climates is also available through GM Dealerships; refer to Specifications for further information. Failure to use the proper power steering fluid can cause power steering hose and seal damage, fluid leaks and pump failure.

3. Fill the fluid reservoir with power steering fluid.
4. Inspect for leaks. If there are leaks, correct the cause of the leaks and bleed the system. Refer to Power Steering System Bleeding .