For 1990-2009 cars

## RPO Code List Hatchback in North America

RPO | Description
--- | ---
04U | Urban Grey (Metallic)
05U | Misty Blue (Mica)
06U | Flame Red (Mica)
11U | Galaxy White (Solid)
33U | Sports Blue (Mica)
41P | Steel Wheel Color - Black
52U | Highway Yellow (Solid)
54U | Sunset Orange (Metallic)
5QC | Door Trim - Front and Rear - Full Formed (Plastic Bare)
5QD | Door Trim - Front and Rear - Full Formed (P/Fabric)
71U | Super Red (Solid)
81I | Charcoal Interior Color
87U | Pearl Black (Mica)
92U | Poly Silver (Metallic)
A02 | Glass - Tinted w/Windshield Top Band
A70 | Seat Belt - Pretensioner, FRT LH/RH
A79 | Front Seat - H/ADJ., Single Type - DRV
AAL | Knee Bolster, DRV and Co-Driver
AC8 | All Tinted Wind Glass
AE3 | Window Operation - PWR, FRT and RR
AHU | FRT Seat Belt Height Adjuster
AJ7 | FRT Airbag, DRV and Co-DRV, Side Airbag, DRV and Co-DRV
AK5 | Airbag, Driver And Co-Driver
AK9 | Seat Belt - 3 Point CLR, RR CTR,OTR
AM1 | Lumber Support - DRV Side
AMA | Second Row Seat - Split Back, D/Folding w/Separated H/Rest
APW | Window Operation - Manual
AR7 | Front Seat - Recliner, Lever Type (Dual Lock)
AT2 | FRT Seat Headrest - w/H/Adjuster (w/Tiltable)
AT3 | Child Seat Tether Anchorage Prov.
AU3 | Lock - Doors, Electric
B19 | Metallic Paint
B37 | Car Mat w/o Logo and w/o Heel Pad (Hook Type)
BAH | Engine Immobilizer
BIH | Hood Insulation
BMF | Badge - Pontiac
BMH | Badge - Suzuki
BUP | Manufacturing Plant - Bupyeong #1, Republic Of Korea
BXQ | Blackout Tape - Pillar Outer
C13 | Windshield Wiper and Washer - 2-Speed w/Intermittent
C25 | Tailgate Wiper and Washer - w/o Intermittent
C35 | Rear Heating Duct
C3Z | T/Gate Glass Defogger, w/o Timer
C46 | Heater w/4-Speed Fan
C49 | T/Gate Glass Defogger, w/Timer
C60 | Integral Air-Con. (R134A)
C66 | Uncompleted Air-Con.
C98 | Airbag, Advanced
C9C | Paint Special, Black (Wheel House Black Painting)
CF5 | Sunroof - Glass, Elec. Tilting
D05 | Arm Rest - DRV Side
D31 | Inside Mirror - Tilt, RR View
D52 | Rear Spoiler w/o CHMSL Sporty 2
D72 | Door Outside Handle - Black
D75 | Door Outside Handle - Body Color
D80 | Rear Spoiler w/o CHMSL Sporty 1
D8R | Guam - Mandatory
D91 | Door Outside Handle - Body Color
D94 | Touchup Paint
DG2 | OSRVM, Turnover Type - Manual Remote - Cable, Driver and Co-Driver
DL6 | OSRVM, Turnover Type - Power Remote, Driver and Co-Driver
DLB | Floor Covering - w/Driver Side Heel Pad
DNJ | Sunshade - w/Mirror, w/o Miirror Cover
DP5 | OSRVM, Turnover Type - Black
DQ9 | OSRVM, Turnover Type - Body Color
DT4 | Ashtray, FRT - w/o Lamp
E19 | Bumper, FRT/RR - 5 mph
E2U | Lettering - Trim Level - "LS" Lettering
E91 | Seat Back Pocket - Co-Driver Side
FE2 | Suspension - Standard
FX1 | Final Transaxle Drive Ratio . 3.944
GH4 | USA - Mandatory
GH5 | Canada - Mandatory
GY5 | Final Transaxle Drive Ratio . 3.750
J41 | Brake - FRT, DISC, RR, Drum
JG0 | Brakes - Front - Vent. Disc (256)
JM4 | Brake - FRT, DISC, RR, Drum ABS
K05 | Engine Block Heater
K11 | Air Filter
K34 | Cruise Control
K99 | Alternator - 85A
KC5 | Extra Power Jack
KD6 | Engine Starter - 1.2 kw
KRD | Octane No. - RON 91
LHD | Vehicle Drive - LHD
LXT | 1.6L DOHC MPI - FAM. I
M97 | Key Interlock System
MLM | MT-5 - DI6 (Semi-Wide)
MLQ | AT-4 - Aisin
MPN | Clutch, Hydraulic Type
N33 | Tiltable Steering Column
N40 | Steering - Power
N44 | Steering Wheel - 4 Spoke, STD (w/Airbag)
NPH | Muffler - Heavy Duty (Warranty 3 Years)
NU2 | Emission - N/America, ULEV III
P2W | Wheel Cover 14 inch (Bolt-On)
PG4 | 14×5.5J Alloy Wheel
PG9 | 15×6.0J Alloy Wheel
PTJ | Remote Key - 2EA
PW8 | 15×6.0J Alloy Wheel
PY8 | 14×5.5J Steel Wheel
Q98 | Tire - 185/60R14
QI0 | Lettering - Trim Level #0
QI1 | Lettering - Trim Level #1
QI2 | Lettering - Trim Level #2
QQ6 | Spare Tire - Temporary (T105/70 D14)
QUK | Tire - 185/55R15
T2C | Equipment - Cold Area
T2Y | Child Seat Lower Anchorage (Fix Prov.)
T5R | Second Row Seat - Locking Control - Safety RR Seat Back
T61 | Day Time Running Light
T73 | Front Lamps - SAE, LHD
T90 | Side Turn Signal Lamp - White
T96 | Front Fog Lamp
TDK | H/Lamp On, Key Reminder, S/Belt Chime Bell
TDW | B.I.W. Panel - Partial Coating
TN6 | Battery - 55AH, 550 CCA
TR1 | Rear Lamps - SAE LHD w/o RR Fog Lamp
TRB | Radiator Grille - Body Color
TS6 | CHMSL (Center High Mounted Stop Lamp)
TTA | Side Markers, Front/Rear
TUL | FRT Turn Signal Lamp - SAE
TUQ | Cigar Lighter - w/o Lamp
U18 | Meter Cluster - Illumination - Translucent - Kilometers (Range 200 kph)
U2D | Meter Cluster - Analogue - Cluster-DLX (w/Tacho)
U71 | Antenna - Passive Type, Roof
UA5 | Anti Theft Device - Car Alarm and Keyless Entry Sys.
UAY | D/Din-Radio and CDP and MP3 and INDASH 6 CDC
UC1 | Meter Cluster - Illumination - Translucent - Miles (Range 120 mph)
UE8 | Digital Clock
UJ9 | TPMS (Tire Air-Pressure Monitoring System)
UK3 | Audio Remote Control
UM7 | Single Din - AM/FM Radio Only
UPX | D/Din - 45Wx4Ch, Radio and CDP (w/MP3)
UQ4 | Speaker - 4EA (FRT/RR STD)
UW6 | Speaker - 6EA (FRT/RR DLX + Tweeter FRT)
VED | Metallic Grain
VEE | Bumper - Body Color
VGC | Wrap Guard
VH4 | Mud Guard
VIX | Visual V.I.N. Plate
VK8 | Sunglass Holder
VNS | VIN Model Year 2008
VNU | VIN Plate - US Type
VOB | Radiatior Grille - Chrome - Lattice Type
W2V | Lettering - Trim Level - No Lettering
W6H | Seat Cover - Full Fabric (DLX.2)
W6N | Seat Cover - Full Fabric (STD)
WAN | Lettering - Car Name - Aveo
WAO | Lettering - Car Name - Wave
WAP | Lettering - Car Name - Swift +
WCM | Lettering - Trim Level - "LT" Lettering
WU5 | Dimmer - Instrument Cluster
Y9Y | Badge - Chevrolet
Z5U | OSRVM, Turnover Type - Heating Function

## RPO Code List Hatchback Outside North America

RPO | Description
--- | ---
04U | Urban Grey (Metallic)
05U | Misty Blue (Mica)
06U | Flame Red (Mica)
11U | Galaxy White (Solid)
2G0 | Singapore - Mandatory
2G1 | Israel - Mandatory
33U | Sports Blue (Mica)
41P | Steel Wheel Color - Black
52U | Highway Yellow (Solid)
54U | Sunset Orange (Metallic)
5QC | Door Trim - Front And Rear - Full Formed (Plastic Bare)
5QD | Door Trim - Front And Rear - Full Formed (P/Fabric)
5TC | Western Samoa - Mandatory
5TI | Ukraine - Mandatory
71U | Super Red (Solid)
81I | Charcoal Interior Color
87U | Pearl Black (Mica)
92U | Poly Silver (Metallic)
A02 | Glass - Tinted w/Windshield Top Band
A03 | Glass - All Clear w/Windshield Top Band
A32 | Window Operation - PWR, FRT
A70 | Seat Belt - Pretensioner, FRT LH/RH
A79 | Front Seat - H/ADJ., Single Type - DRV
AA6 | All Clear Wind Glass
AAM | Knee Bolster, Driver Side
AC8 | All Tinted Wind Glass
AE3 | Window Operation - PWR, FRT and RR
AHU | FRT Seat Belt Height Adjuster
AIA | Seat Belt - 3 Point ELR, FRT, Co-Driver Side
AIB | Seat Belt - Belt-FRT Co-DR 3P ELR, L/L
AIF | Seat Belt - Belt-FRT DR, 3P ELR, L/L
AIG | Seat Belt - 3 Point ELR, FRT, Driver Side
AJ3 | Airbag, Driver Only
AJ7 | FRT Airbag, DRV and Co-DRV, Side Airbag, DRV and Co-DRV
AK5 | Airbag, Driver and Co-Driver
AK7 | Seat Belt - 2 Point Manual, RR CTR
ALU | Second Row Seat - Seat - RR, FolDINg w/Headrest (3EA) - FolDINg
AM7 | Second Row Seat - 1 Piece Back, D/FolDINg w/Integrated H/Rest
AMA | Second Row Seat - Split Back, D/FolDINg w/Separated H/Rest
APW | Window Operation - Manual
AQ6 | Front Seat - Recliner, Lever Type
AR1 | Airbag, Delete
AR7 | Front Seat - Recliner, Lever Type (Dual Lock)
AR9 | Front Seat - Recliner, Dial Type
AT2 | FRT Seat Headrest - W/H/Adjuster (W/Tiltable)
AT3 | Child Seat Tether Anchorage Prov.
AT7 | Seat Belt - 3 Point ELR, RR CTR
AUG | Lock - Doors, Electric
AWG | Seat Belt - 3 Point ELR, RR OTR
B00 | Indonesia - Mandatory
B02 | South Africa - Mandatory
B03 | Thailand - Mandatory
B04 | Taiwan - Mandatory
B09 | Egypt - Mandatory
B10 | Malaysia - Mandatory
B12 | Russia - Mandatory
B13 | Australia - Mandatory
B14 | Hong Kong - Mandatory
B15 | Philippine - Mandatory
B19 | Metallic Paint
B37 | Car Mat w/o Logo and w/o Heel Pad (Hook Type)
B56 | Rocker MolDINg
BAH | Engine Immobilizer
BIH | Hood Insulation
BLQ | ID Plate Type "A"
BLS | ID Plate Type "B"
BLV | ID Plate Type "D"
BLW | ID Plate Type "E"
BMC | ID Plate Type "H-1"
BMS | ID Plate Delete
BPZ | ID Plate Type "T"
BUP | Manufacturing Plant - Bupyeong #1, Republic Of Korea
BW2 | Body Side MolDINg
BXQ | Blackout Tape - Pillar Outer
C13 | Windshield Wiper and Washer - 2-Speed w/Intermittent
C16 | Tailgate Wiper and Washer - w/Intermittent
C25 | Tailgate Wiper and Washer - w/o Intermittent
C35 | Rear Heating Duct
C3Z | T/Gate Glass Defogger, w/o Timer
C46 | Heater w/4-Speed Fan
C60 | Integral Air-Con. (R134A)
C66 | Uncompleted Air-Con.
C9C | Paint Special, Black (Wheel House Black Painting)
CAI | Rear Lamps - ECE w/o RR Fog Lamp
CB7 | Colombia - Mandatory
CF5 | Sunroof - Glass, Elec. Tilting
CGK | Libya - Mandatory
CK1 | Pakistan - Mandatory
CK2 | Yemen
CR8 | Egypt
CR9 | Morocco
CS1 | Tunisia
CS2 | Nigeria
CS5 | Angola
CS6 | Ethiopia
CU7 | Kuwait
CU8 | Saudi Arabia
CV4 | Israel
CV8 | Iraq
CX8 | Syria
CX9 | Lebanon
CY2 | Jordan
CY3 | Cameroon
CY4 | Ivory Coast
CY6 | Gabon
D1K | Clutch, Cable Type
D2G | Algeria
D2J | Guinea
D2K | Grenada
D2L | St. Lucia
D2O | Curacao
D2U | Guyana
D2Y | Antigua
D31 | Inside Mirror - Tilt, RR View
D3B | Bermuda
D3D | Trinidad and Tobago
D3E | Eritrea
D3G | Cape Verde
D3I | Barbados
D3J | Cayman Is.
D3K | Dominican Rep.
D3L | El Salvador
D3M | Guatemala
D3P | Haiti
D3Q | Honduras
D3R | Jamaica
D3S | Qatar
D3U | St. Maarten
D4C | Bahrain
D4G | Bahamas
D4H | Belize
D4N | Costa Rica
D4X | Aruba
D5D | Nicaragua
D5F | Senegal
D5K | Surinam
D5P | U.A.E
D6F | Congo
D72 | Door Outside Handle - Black
D75 | Door Outside Handle - Body Color
D7J | Seat Back Picnic Table (Co-Driver Side Only)
D80 | Rear Spoiler w/o CHMSL Sporty 1
D8S | Iraq - Mandatory
D8T | Iran - Mandatory
D8U | Jordan - Mandatory
D8V | Kazakhstan - Mandatory
D8X | Lebanon - Mandatory
D91 | Door Outside Handle - Body Color
D94 | Touchup Paint
DG2 | OSRVM, Turnover Type - Manual Remote - Cable, Driver and Co-Driver
DL6 | OSRVM, Turnover Type - Power Remote, Driver and Co-Driver
DLB | Floor Covering - w/Driver Side Heel Pad
DNB | OSRVM, Turnover Type - Manual Remote Cable - Driver, Power Remote Co-Driver
DNJ | Sunshade - w/Mirror, w/o Miirror Cover
DP5 | OSRVM, Turnover Type - Black
DQ9 | OSRVM, Turnover Type - Body Color
DQB | Mirror I/S R/V - w/o Tilt
DT4 | Ashtray, FRT - w/o Lamp
E17 | Bumper, FRT/RR - 2.5 mph
E2U | Lettering - Trim Level - "LS" Lettering
E46 | Ecuador - Mandatory
E6G | Ghana
E6H | Oman
E7B | Liberia
E7C | Libya
E7E | Madagascar
E7J | Mauritius
E7Q | British Virgin Is.
E7W | Fire Extinguisher w/Bracket
E90 | Seat Back Pocket - Driver Side
E91 | Seat Back Pocket - Co-Driver Side
EF2 | Guinea-Bissau
EF5 | Panama
ELH | Seat Side Pocket - Co-Driver Side
ERI | Battery Saver
ET8 | Syria - Mandatory
F77 | Final Transaxle Drive Ratio . 4.105
FE2 | Suspension - Standard
FG3 | Gas Shock Absorbor
FQ7 | Final Transaxle Drive Ratio . 4.052
FV1 | Final Transaxle Drive Ratio . 3.722
FV2 | Final Transaxle Drive Ratio . 4.176
FWL | Final Transaxle Drive Ratio . 4.444
FX1 | Final Transaxle Drive Ratio . 3.944
GFM | Equipment Regional ; General
GFP | Equipment Regional ; Australia
GFS | Equipment Regional ; Gulf States
GH3 | Saudi Arabia - Mandatory
GY5 | Final Transaxle Drive Ratio . 3.750
HDN | Badge - Holden
J41 | Brake - FRT, DISC, RR, Drum
JA3 | Parking Brake Button - Chrome
JF2 | Brakes - Front - Vent. Disc (236)
JG0 | Brakes - Front - Vent. Disc (256)
JM4 | Brake - FRT, DISC, RR, Drum ABS
K11 | Air Filter
K35 | Equipment - High Altitude
K36 | Equipment - Low Volatility Fuel
K97 | Alternator - 80A
K99 | Alternator - 85A
KC5 | Extra Power Jack
KD6 | Engine Starter - 1.2 kw
KD7 | Engine Starter - 0.8 kw
KE1 | Chile - Mandatory
KIM | Lettering - Trim Level - "SE" Lettering
KIX | Lettering - Trim Level - "SX" Lettering
KRB | Octane No. - RON 83
KRC | Octane No. - RON 87
KRD | Octane No. - RON 91
KRE | Octane No. - RON 95
L95 | 1.4L DOHC MPI - FAM. I
LBJ | 1.4L SOHC MPI - FAM. I
LHD | Vehicle Drive - LHD
LV8 | 1.5L SOHC MPI - FAM. I
LXT | 1.6L DOHC MPI - FAM. I
LY4 | 1.2L SOHC MPI - T4
MFG | MT-5 - Y4M
MFH | MT-5 - D16 (Modify C/R)
MLL | MT-5 - DI6 (W/R)
MLM | MT-5 - DI6 (Semi-Wide)
MLQ | AT-4 - Aisin
MPN | Clutch, Hydraulic Type
MTF | Bracket, Fire Extinguisher
N12 | Muffler - Standard (Warranty 2 Years)
N33 | Tiltable Steering Column
N40 | Steering - Power
N44 | Steering Wheel - 4-Spoke, STD (w/Airbag)
N45 | Steering Wheel - 3-Spoke (w/o Airbag)
N51 | Steering - Manual
NF1 | N/America, LEV
NPH | Muffler - Heavy Duty (Warranty 3 Years)
NQN | Emission - Korea 2000
NQS | Emission - Korea 90 (US83)
NQT | Emission - OP/Loop, Leaded
NR0 | Steering WHL - Leather, 4 SPK
NT2 | Emission - EURO II
NT3 | Emission - EURO III
NT4 | Emission - EURO IV
P2W | Wheel Cover 14 inch (Bolt-On)
PB0 | Wheel Cover 13 inch (Wire)
PB1 | Wheel Cover 15 inch (Bolt-On )
PG1 | 15×6.0J Steel Wheel
PG4 | 14×5.5J Alloy Wheel
PG9 | 15×6.0J Alloy Wheel
PTJ | Remote Key - 2EA
PW8 | 15×6.0J Alloy Wheel
PY8 | 14×5.5J Steel Wheel
PZC | 13×5.0J Steel Wheel
Q98 | Tire - 185/60R14
QDX | Tire - 155/80R13
QI0 | Lettering - Trim Level #0
QI1 | Lettering - Trim Level #1
QI2 | Lettering - Trim Level #2
QQ5 | Spare Tire - Regular, Steel
QQ6 | Spare Tire - Temporary (T105/70 D14)
QUK | Tire - 185/55R15
RHD | Vehicle Drive - RHD
T2C | Equipment - Cold Area
T2Y | Child Seat Lower Anchorage (Fix Prov.)
T44 | Speed Warning, Chime Bell
T5R | Second Row Seat - Locking Control - Safety RR Seat Back
T61 | Day Time Running Light
T84 | Front Lamps - ECE, LHD
T85 | Front Lamps - ECE, RHD
T90 | Side Turn Signal Lamp - White
T96 | Front Fog Lamp
T9E | Rear Lamps - ECE w/RR Fog Lamp
TB1 | Rear Lamps - Domestic
TCU | License Plate Bracket, FRT - Large : ECE
TDK | H/Lamp On, Key Reminder, S/Belt Chime Bell
TDW | B.I.W. Panel - Partial Coating
TN6 | Battery - 55AH, 550 CCA
TP4 | Battery - 45AH, 430 CCA
TR6 | Front Lamps - Leveling Device, H/Lamp - ECE
TS6 | CHMSL (Center High Mounted Stop Lamp)
TUQ | Cigar Lighter - w/o Lamp
TYR | Leather Package (Steering WHL, G/Knob)
TZB | E-Model Package
U17 | Meter Cluster - Analogue - Cluster-STD (w/o Tacho)
U18 | Meter Cluster - Illumination - Translucent - Kilometers (Range 200 kph)
U2D | Meter Cluster - Analogue - Cluster-DLX (w/Tacho)
U71 | Antenna - Passive Type, Roof
UA5 | Anti Theft Device - Car Alarm and Keyless Entry Sys.
UAK | AM/FM Radio and CDP (w/o MP3)
UAL | Single DIN - RDS
UC1 | Meter Cluster - Illumination - Translucent - Miles (Range 120 mph)
UE8 | Digital Clock
UK3 | Audio Remote Control
UK5 | Single DIN - Cassette, H/PWR, 4 CH, 4 SPK, Mech Deck
UPK | AM/FM Radio and CDP (w/MP3)
UPR | D/DIN - 45Wx4Ch, Logic/EQ/CDP/MP3
UPT | Single DIN - Cassette, H/PWR, 4 CH, 4 SPK, Logic Deck
UPU | D/DIN - 45Wx4CH, Logic/EQ
UPX | D/DIN - 45Wx4CH, Radio and CDP (w/MP3)
UPY | CDC, Double DIN - 5 CDC, 6 SPK
UQ4 | Speaker - 4EA (FRT/RR STD)
UQD | D/DIN-Radio and Tape and CDP and MP3 and INDASH 6 CDC
UW6 | Speaker - 6EA (FRT/RR DLX+Tweeter FRT)
VEE | Bumper - Body Color
VFT | B.I.W. Panel - Uncoated
VGC | Wrap Guard
VH4 | Mud Guard
VGIX | Visual V.I.N. Plate
VIY | VIN Plate - Asterimark(*)
VK8 | Sunglass Holder
VMB | Bumper FRT - Molded, All
VNR | VIN Model Year 2007
VNS | VIN Model Year 2008
VNT | VIN Model Year 2009
VNU | VIN Plate - US Type
VNW | VIN Plate - EURO Type
VOB | Radiatior Grille - Chrome - Lattice Type
VPQ | Wax Remover
VTW | Deposit Box - Passenger Side, I/P Upper
W2V | Lettering - Trim Level - No Lettering
W6H | Seat Cover - Full Fabric (DLX.2)
W6N | Seat Cover - Full Fabric (STD)
WAL | Lettering - Car Name - Aveo
WAN | Lettering - Car Name - Aveo
WAQ | Lettering - Car Name - Kalos
WCM | Lettering - Trim Level - "LT" Lettering
WU5 | Dimmer - Instrument Cluster
XA6 | ECE Label
XP7 | Lettering - Car Name - Barina
XX7 | Single DIN - Blind Cover w/o Cassette, 4 Spk
XXX | Single DIN - Blind Cover w/o Cassette, 4 Spk w/Audio Frame
XZ1 | Equipment - Hot Area
Y9Y | Badge - Chevrolet
Z5U | OSRVM, Turnover Type - Heating Function

## RPO Code List Notchback in North America

RPO | Description
--- | ---
04U | Urban Grey (Metallic)
05U | Misty Blue (Mica)
06U | Flame Red (Mica)
11U | Galaxy White (Solid)
33U | Sports Blue (Mica)
41P | Steel Wheel Color - Black
52U | Highway Yellow (Solid)
54U | Sunset Orange (Metallic)
5QC | Door Trim Center Parts - Plastic Bare
5QD | Door Trim Center Parts - Fabric - Woven
60I | Interior Color - 2 Tone (Beige+Charcoal)
71U | Super Red (Solid)
81I | Interior Color - Mono Tone (Chacoal)
87U | Pearl Black (Mica)
92U | Poly Silver (Metallic)
A02 | Glass - Tinted W/Windshield Top Band
A03 | Glass - All Clear W/Windshield Top Band
A32 | Window Operation - PWR, FRT
A70 | Seat Belt - Pretensioner, FRT LH/RH
A79 | Front Seat - H/ADJ., Single Type - Driver Side
AA6 | Glass - All Clear Wind Glass
AAL | Knee Bolster, DRV and Co-Driver
AAM | Knee Bolster, Driver Side
AC8 | All Tinted Wind Glass
AE3 | Window Operation - PWR, FRT and RR
AHU | FRT Seat Belt Height Adjuster
AIA | Seat Belt - 3 Point ELR, FRT, Co-Driver Side
AIG | Seat Belt - 3 Point ELR, FRT, Driver Side
AJ7 | SRS Airbag - FRT Airbag, DRV and Co-DRV, Side Airbag, DRV and Co-DRV
AK5 | SRS Airbag - Driver and Co-Driver
AK9 | Seat Belt - 3 Point CLR, RR CTR, OTR
AM1 | Front Seat - Lumbar Support - Driver Side
AMA | Rear Seat - Split Folding s/Back, w/Separated h/Rest
APW | Window Operation - Manual
AR1 | SRS Airbag - Airbag, Delete
AR7 | Front Seat - Recliner, Lever Type (Dual Lock)
AT2 | FRT Seat Headrest - w/H/Adjuster (w/Tiltable)
AT3 | Child Seat Tether Anchorage Prov.
AT7 | Seat Belt - 3 Point ELR, RR CTR
AU3 | Lock - Doors, Electric
AWG | Seat Belt - 3 Point ELR, RR OTR
B1G | Lettering - Car Name - G3
B37 | Car Mat w/o Logo and Pad (Hook Type)
BAH | Engine Immobilizer
BC1 | Instrumental Panel - 2 Piece Plastic, UPR Normal Paint
BC2 | Decoration Pack-III (Beige)
BIH | Hood Insulation
BJ0 | Instrumental Panel - 2 Piece Plastic, UPR PU Paint
BLW | ID Plate Type "E"
BMF | Badge - Pontiac
BQI | Ventilator Grille - Round Type w/Chrome
BUP | Manufacturing Plant - Bupyeong #1, Republic Of Korea
BXP | Door Trim - PU Leather (Beige)
BXQ | B-Pillar Outer - Black Tape
C13 | Windshield Wiper and Washer - 2 Speed w/Intermittent
C1V | Decoration Pack-II
C35 | HVAC - Rear Heating Duct
C46 | HVAC - Heater w/4-Speed Fan
C49 | Back Glass Defogger, w/Timer
C60 | HVAC - Integral Air-Con. (R134A)
C98 | Advanced Air-Bag
C9C | Paint Special, Black (Wheel House Black Painting)
CF5 | Sunroof - Glass, Elec. Tilting
D05 | Front Seat - Armrest, Driver Side
D07 | Floor Console w/o Arm Rest - Silver
D31 | Inside Mirror - Tilt, RR View
D55 | Floor Console w/o Arm Rest - Resin
D75 | Grip Type O/S Handle - Body Color
D8R | Guam - Mandatory
D91 | Rear End Closure - Body Color
DG2 | OSRVM, Turnover Type - Manual Remote - Cable, Driver and Co-Driver
DL6 | OSRVM, Turnover Type - Power Remote, Driver and Co-Driver
DLB | Floor Covering - w/Driver Side Heel Pad
DNJ | Sunvisor - DRV. w/Mirror and w/o Cover, PASS. w/Mirror and w/o Cover
DP5 | OSRVM - Black Color
DQ9 | OSRVM - Body Color
DT4 | Ashtray, FRT - w/o Lamp
DW0 | Cluster Color - Silver Ring
E11 | Mexico - Mandatory
E17 | Bumper, FRT/RR - 2.5 mph
E19 | Bumper, FRT/RR - 5.0 mph
E20 | Grip Type O/S Handle - Chrome Coating
E2U | Lettering - Trim Level - "LS" Lettering
E3E | Trunk Handle - Chrome
E90 | Seat Back Pocket - Driver Side
E91 | Seat Back Pocket - Passenger Side
ELH | Seat Side Pocket - Passenger Side
ERI | Battery Saver
FE2 | Suspension - Standard
FX1 | Final Transaxle Drive Ratio - 3.944 (for 1.4/1.5/1.6L MT)
GFM | Equipment Regional ; General
GH4 | USA - Mandatory
GH5 | Canada - Mandatory
GY5 | Final Transaxle Drive Ratio - 3.750 (for 1.2/1.5/1.6L AT)
J41 | Brake System - FRT DISC and RR Drum, w/o ABS
JF2 | Brake System - Front - Vent. Disc Size - 236
JG0 | Brake System - Front - Vent. Disc Size - 256
JM4 | Brake System - FRT DISC and RR Drum, w/ABS
K05 | Engine Block Heater
K11 | HVAC - Air Filter
K34 | Cruise Control
K99 | Alternator - 85A
KC5 | Extra Power Jack
KD6 | Engine Starter - 1.2kw
KRD | Octane No. - Ron 91
LHD | Vehicle Drive - Left-Hand Drive
LXT | Engine - 1.6L DOHC MPI - FAM I
M97 | Key Interlock System
MLM | Transmission - MT-5 - D16
MLQ | Transmission - AT-4 - Aisin AW (N/A for EURO III or IV w/1.2S)
MPN | Clutch, Hydraulic Type
N33 | Tiltable Steering Column
N40 | Steering - Power
N44 | Steering Wheel - w/Airbag, J200 Type
N45 | Steering Wheel - w/o Airbag, T200 Type
NF1 | Emission - N/America, LEV
NPH | Muffler - Heavy Duty (Warranty 3 Years)
NU2 | Emission - N/America, ULEVII and OBD II
P2W | Wheel Cover - 14 inch
PG9 | Wheel - 15X6J Alloy Wheel (DW/Chevy/Holden)
PTJ | Remote Key - 2EA
PW8 | Wheel - 15×6J Alloy Wheel (Pontiac/Chevrolet)
PY8 | Wheel - 14×5.5J Steel Wheel
Q98 | Tire - 185/60R14
QI0 | Lettering - Trim Level #0
QI1 | Lettering - Trim Level #1
QI2 | Lettering - Trim Level #2
QQ5 | Spare Tire - Regular, Steel
QQ6 | Spare Tire - Temporary (T105/70D14)
QUK | Tire - 185/55R15
T2C | Equipment - Cold Area
T2Y | Child Seat Lower Anchorage (ISOFIX Prov.)
T43 | Trunk Lid Mounted Spoiler (Including LED Lamp)
T61 | Daytime Running Light
T73 | Headlamp With Turn Signal Lamp - SAE, LHD (w/FR/S/Marker)
T90 | Side Turn Signal Lamp - White Color
T96 | Front Fog Lamp
TDK | Warning Device - H/Lamp On, Key Reminder, S/Belt Chime Bell
TDW | B.I.W. Panel - Partial Coating
TN6 | Battery - 55AH,550 CCA
TR1 | RR COMBI. Lamp - Red OTR Lens, SAE w/RR S/Maker
TS6 | CHMSL (Center High Mounted Stop Lamp)
TUQ | Cigar Lighter - w/o Lamp
U18 | Speedometer - Kilometers (Range 200 kph)
U2D | Cluster (w/Tacho) Chevrolet - 4 Circle Type, Pontiac - 3 Circle Type
U77 | Antenna - Wire Type, Back Glass
UA5 | Anti Theft Device - Car Alarm and Keyless Entry w/Trunk Release
UAY | Audio System - Radio, CDC w/MP3 - Black Tie Size
UC1 | Speedometer - Miles (Range 120 mph)
UE8 | Digital Clock
UJ9 | TPMS (Tire Air-Pressure Monitoring System)
UK3 | Remote Audio Steering Controls
UM7 | Audio System - Radio Only - Black Tie Size
UPX | Audio System - Radio, CDP w/MP3 - Black Tie Size
UQ4 | Speaker - 4 Speaker
UW6 | Speaker - 6 Speaker
VA8 | Label - Spanish
VED | Decoration Pack-IV (Charcoal)
VEE | Bumper, FRT/RR - Body Color
VGC | Wrap Guard
VH4 | Mud Guard
VIX | Visual V.I.N. Plate
VK8 | Sunglasses Holder
VNS | VIN Model Year 2008
VNU | VIN Plate - Us Type
VOB | Radiator Grille - Chrome
VPQ | Wax Remover
W1I | Seat Cover - PU Leather (Beige)
W2V | Lettering - Trim Level - No Lettering
W6B | Seat Cover - Fabric - Woven, STD
W6G | Seat Cover - Fabric - Woven, DLX
WAL | Lettering - Car Name - Aveo
WAO | Lettering - Car Name - Wave
WCM | Lettering - Trim Level - "LT" Lettering
WU5 | Dimmer - Instrument Cluster
Y9Y | Badge - Chevrolet
Z5U | OSRVM, Turnover Type - Heating Function

## RPO Code List Notchback Outside North America

RPO | Description
--- | ---
04U | Urban Grey (Metallic)
05U | Misty Blue (Mica)
06U | Flame Red (Mica)
11U | Galaxy White (Solid)
2G0 | Singapore - Mandatory
2G1 | Israel - Mandatory
33U | Sports Blue (Mica)
41P | Steel Wheel Color - Black
52U | Highway Yellow (Solid)
54U | Sunset Orange (Metallic)
5QC | Door Trim Center Parts - Plastic Bare
5QD | Door Trim Center Parts - Fabric - Woven
5TC | Western Samoa - Mandatory
5TD | Yemen - Mandatory
5TI | Ukraine - Mandatory
60I | Interior Color - 2 Tone (Beige+Charcoal)
71U | Super Red (Solid)
81I | Interior Color - Mono Tone (Charcoal)
87U | Pearl Black (Mica)
92U | Poly Silver (Metallic)
A02 | Glass - Tinted w/Windshield Top Band
A03 | Glass - All Clear w/Windshield Top Band
A32 | Window Operation - PWR, FRT
A70 | Seat Belt - Pretensioner, FRT LH/RH
A79 | Front Seat - H/ADJ., Single Type - Driver Side
AA6 | Glass - All Clear Wind Glass
AAM | Knee Bolster, Driver Side
ABZ | Window Operation - PWR, FRT and RR w/FRT. One Touch Down and Up (Driver Side)
AC8 | All Tinted Wind Glass
AE3 | Window Operation - PWR, FRT and RR
AHU | FRT Seat Belt Height Adjuster
AIA | Seat Belt - 3 Point ELR, FRT, Co-Driver Side
AIB | Seat Belt - Belt-FRT Co-DR 3P ELR, L/L
AIF | Seat Belt - Belt-FRT, DR, 3P ELR, L/L
AIG | Seat Belt - 3 Point ELR, FRT, Driver Side
AJ3 | SRS Airbag - Driver Only
AJ7 | SRS Airbag - FRT Airbag, DRV and Co-DRV, Side Airbag, DRV and Co-DRV
AK5 | SRS Airbag - Driver and Co-Driver
AK7 | Seat Belt - 2 Point Manual, RR CTR
ALU | Rear Seat - Split Folding S/Back, w/Separated H/Rest (3EA)
AMA | Rear Seat - Split Folding S/Back, w/Separated H/Rest
AN1 | Rear Seat - Fixed S/Back, w/Integrated H/Rest
APW | Window Operation - Manual
AQ6 | Front Seat - Recliner, Lever Type
AR1 | SRS Airbag - Airbag, Delete
AR7 | Front Seat - Recliner, Lever Type (Dual Lock)
AR9 | Front Seat - Recliner, Dial Type
AT2 | FRT Seat Headrest - w/H/Adjuster (w/Tiltable)
AT3 | Child Seat Tether Anchorage Prov.
AT7 | Seat Belt - 3 Point ELR, RR CTR
AU3 | Lock - Doors, Electric
AWG | Seat Belt - 3 Point ELR, RR OTR
B00 | Indonesia - Mandatory
B02 | South Africa - Mandatory
B03 | Thailand - Mandatory
B04 | Taiwan - Mandatory
B09 | Egypt - Mandatory
B10 | Malaysia - Mandatory
B12 | Russia - Mandatory
B13 | Australia - Mandatory
B14 | Hong Kong - Mandatory
B15 | Philippine - Mandatory
B1G | Lettering - Car Name - G3
B37 | Car Mat w/o Logo and Pad (Hook Type)
BAH | Engine Immobilizer
BC1 | Instrumental Panel - 2 Piece Plastic, UPR Normal Paint
BC2 | Decoration Pack-III (Beige)
BIH | Hood Insulation
BLQ | ID Plate Type "A"
BLS | ID Plate Type "B"
BLV | ID Plate Type "D"
BLW | ID Plate Type "E"
BLY | ID Plate Type "F"
BMC | Plate Inscription Type 'h-1'
BMF | Badge - Pontiac
BMS | ID Plate Delete
BPZ | ID Plate Type "T"
BQI | Ventilator Grille - Round Type w/Chrome
BUP | Manufacturing Plant - Bupyeong #1, Republic Of Korea
BXQ | B-Pillar Outer - Black Tape
C13 | Windshield Wiper and Washer - 2 Speed w/Intermittent
C1V | Decoration Pack-II
C35 | HVAC - Rear Heating Duct
C46 | HVAC - Heater w/4-Speed Fan
C49 | Back Glass Defogger, w/Timer
C60 | HVAC - Integral Air-Con. (R134A)
C66 | HVAC - Uncompleted Air-Con.
C68 | HVAC - FATC (Full Auto Temperature Control)
C99 | SRS Airbag - Passenger Airbag, Manual Cut-Off
C9C | Paint Special, Black (Wheel House Black Painting)
CAI | Rear Lamps - Red OTR Lens, ECE w/o RR Fog Lamp
CF5 | Sunroof - Glass, Elec. Tilting
CGK | Libya - Mandatory
CK1 | Pakistan - Mandatory
CK2 | Yemen
CR8 | Egypt
CR9 | Morocco
CS1 | Tunisia
CS2 | Nigeria
CS5 | Angola
CS6 | Ethiopia
CU7 | Kuwait
CU8 | Saudi Arabia
CV4 | Israel
CV8 | Iraq
CX8 | Syria
CX9 | Lebanon
CY2 | Jordan
CY3 | Cameroon
CY4 | Ivory Coast
CY6 | Gabon
D05 | Front Seat - Armrest, Driver Side
D07 | Floor Console w/o Arm Rest - Silver
D1K | Clutch, Cable Type
D2G | Algeria
D2J | Guinea
D2K | Grenada
D2L | St.Lucia
D2O | Curacao
D2U | Guyana
D2Y | Antigua
D31 | Inside Mirror - Tilt, RR View
D3B | Bermuda
D3D | Trinidad and Tobago
D3E | Eritrea
D3G | Cape Verde
D3I | Barbados
D3J | Cayman Is.
D3K | Dominican Rep.
D3L | El Salvador
D3M | Guatemala
D3P | Haiti
D3Q | Honduras
D3R | Jamaica
D3S | Qatar
D3U | St. Maarten
D4C | Bahrain
D4G | Bahamas
D4H | Belize
D4N | Costa Rica
D4X | Aruba
D55 | Floor Console w/o Arm Rest - Resin
D59 | Spoiler - RR, Integ. Decklid
D5D | Nicaragua
D5F | Senegal
D5K | Surinam
D5P | U.A.E
D6F | Congo
D72 | Grip Type O/S Handle - Black Color
D75 | Grip Type O/S Handle - Body Color
D8S | Iraq - Mandatory
D8T | Iran - Mandatory
D8U | Jordan - Mandatory
D8V | Kazakhstan - Mandatory
D8X | Lebanon - Mandatory
D91 | Rear End Closure - Body Color
D94 | Touchup Paint
DG2 | OSRVM, Turnover Type - Manual Remote - Cable, Driver and Co-Driver
DL6 | OSRVM, Turnover Type - Power Remote, Driver and Co-Driver
DLB | Floor Covering - w/Driver Side Heel Pad
DNJ | Sunvisor - DRV. w/Mirror and w/o Cover, PASS. w/Mirror and w/o Cover
DP5 | OSRVM - Black Color
DQ9 | OSRVM - Body Color
DQB | Inside Mirror - Conventional
DT4 | Ashtray, FRT - w/o Lamp
DW0 | Cluster Color - Silver Ring
E11 | Mexico - Mandatory
E17 | Bumper, FRT/RR - 2.5 mph
E20 | Grip Type O/S Handle - Chrome Coating
E2U | Lettering - Trim Level - "LS" Lettering
E3E | Trunk Handle - Chrome
E46 | Ecuador - Mandatory
E6G | Ghana
E6H | Oman
E7B | Liberia
E7C | Libya
E7E | Madagascar
E7J | Mauritius
E7Q | British Virgin Is.
E7W | Fire Extinguisher w/Bracket
E90 | Seat Back Pocket - Driver Side
E91 | Seat Back Pocket - Passenger Side
EF2 | Guinea-Bissau
EF5 | Panama
ELH | Seat Side Pocket - Passenger Side
ERI | Battery Saver
ET8 | Syria - Mandatory
F77 | Final Transaxle Drive Ratio - 4.105 (for 1.2L MT)
FE2 | Suspension - Standard
FG3 | Suspension - Gas Shock Absorbor
FQ7 | Final Transaxle Drive Ratio - 4.052 (for 1.4L AT)
FV1 | Final Transaxle Drive Ratio - 3.722 (for 1.5L MT)
FX1 | Final Transaxle Drive Ratio - 3.944 (for 1.4/1.5/1.6L MT)
GFM | Equipment Regional ; General
GFP | Equipment Regional ; Australia
GFS | Equipment Regional ; Gulf States
GH3 | Saudi Arabia - Mandatory
GY5 | Final Transaxle Drive Ratio - 3.750 (for 1.2/1.5/1.6L AT)
HDN | Badge - Holden (LION)
J41 | Brake System - FRT DISC and RR Drum, w/o ABS
JF2 | Brake System - Front - Vent. Disc Size - 236
JG0 | Brake System - Front - Vent. Disc Size - 256
JM4 | Brake System - FRT DISC and RR Drum, w/ABS
K11 | HVAC - Air Filter
K35 | Equipment - High Altitude
K36 | Equipment - Low Volatile
K97 | Alternator - 80A
K99 | Alternator - 85A
KC5 | Extra Power Jack
KD6 | Engine Starter - 1.2 kw
KD7 | Engine Starter - 0.8 kw
KE1 | Chile - Mandatory
KRB | Octane No. - RON 83
KRC | Octane No. - RON 87
KRD | Octane No. - RON 91
KRE | Octane No. - RON 95
L95 | Engine - 1.4L DOHC MPI - FAM I
LHD | Vehicle Drive - Left-Hand Drive
LV8 | Engine - 1.5L SOHC MPI - FAM I
LXT | Engine - 1.6L DOHC MPI - FAM I
LY4 | Engine - 1.2L SOHC MPI - T4
M97 | Key Interlock System
MFG | Transmission - MT-5 - Y4M
MLM | Transmission - MT5 - D16
MLQ | Transmission - AT-4 - Aisin AW (N/A for EURO III or IV W/1.2S)
MPN | Clutch, Hydraulic Type
MTF | Bracket, Fire Extinguisher
N12 | Muffler - Standard (Warranty 2 Years)
N33 | Tiltable Steering Column
N40 | Steering - Power
N44 | Steering Wheel - w/Airbag, J200 Type
N45 | Steering Wheel - w/o Airbag, T200 Type
N51 | Steering - Manual
NF1 | Emission - N/America, LEV
NPH | Muffler - Heavy Duty (Warranty 3 Years)
NQN | Emission - Korean 2000
NQS | Emission - Korea 90 (US83)
NQT | Emission - Leaded, Op/Loop (ECE83)
NR0 | Steering Wheel - Leather, 4 Spokes
NT2 | Emission - EURO II (ECE96)
NT3 | Emission - EURO III (2000)
NT4 | Emission - EURO IV (2005)
P2W | Wheel Cover - 14 inch
PB0 | Wheel Cover - 13 inch
PB1 | Wheel Cover - 15 inch
PG1 | Wheel - 15×6J Steel Wheel
PG4 | Wheel - 14X5.5J Alloy Wheel
PG9 | Wheel - 15X6J Alloy Wheel (DW/Chevy/Holden)
PTJ | Remote Key - 2EA
PW8 | Wheel - 15×6J Alloy Wheel (Pontiac/Chevrolet)
PY8 | Wheel - 14×5.5J Steel Wheel
PZC | Wheel - 13×5.0J Steel Wheel
Q98 | Tire - 185/60R14
QDX | Tire - 155/80R13
QI0 | Lettering - Trim Level #0
QI1 | Lettering - Trim Level #1
QI2 | Lettering - Trim Level #2
QQ5 | Spare Tire - Regular, Steel
QQ6 | Spare Tire - Temporary (T105/70D14)
QUK | Tire -185/55R15
RHD | Vehicle Drive - Right-Hand Drive
T2C | Equipment - Cold Area
T2Y | Child Seat Lower Anchorage (ISOFIX Prov.)
T43 | Trunk Lid Mounted Spoiler (Including LED Lamp)
T44 | Warning Device - Speed Warning, Chime Bell
T61 | Daytime Running Light
T73 | Headlamp with Turn Signal Lamp - SAE, LHD (w/ FR/S/Marker)
T84 | Headlamp with Turn Signal Lamp - ECE, LHD
T85 | Headlamp with Turn Signal Lamp - ECE, RHD
T90 | Side Turn Signal Lamp - White Color
T96 | Front Fog Lamp
T9E | RR COMBI. Lamp - Red OTR Lens, ECE w/RR Fog Lamp
TB1 | RR COMBI. Lamp - Red OTR Lens, Domestic
TCU | License Plate Bracket, FRT - Large : ECE
TDK | Warning Device - H/Lamp On, Key Reminder, S/Belt Chime Bell
TDW | B.I.W. Panel - Partial Coating
TN6 | Battery - 55AH, 550 CCA
TP4 | Battery - 45AH, 430 CCA
TR1 | RR COMBI. Lamp - Red OTR Lens, SAE w/RR S/Maker
TR6 | H/Lamp Leveling Device (ECE Type Only)
TS6 | CHMSL (Center High Mounted Stop Lamp)
TUQ | Cigar Lighter - w/o Lamp
TYR | Leather Package (Steering WHL, G/Knob)
U18 | Speedometer - Kilometers (Range 200 kph)
U2D | Cluster (w/Tacho) Chevrolet - 4 Circle Type, Pontiac - 3 Circle Type
U68 | Trip Computer
U77 | Antenna - Wire Type, Back Glass
UA5 | Anti Theft Device - Car Alarm and Keyless Entry w/Trunk Release
UAL | Audio System - RDS Function
UAY | Audio System - Radio, CDC w/MP3 - Black Tie Size
UC1 | Speedometer - Miles (Range 120 mph)
UE8 | Digital Clock
UK3 | Remote Audio Steering Controls
UPT | Audio System - Radio/Cassette - Black Tie Size
UPX | Audio System - Radio, CDP w/MP3 - Black Tie Size
UQ4 | Speaker - 4 Speaker
UQD | Audio System - Radio, Cassette, CDC w/MP3 - Black Tie Size
UW6 | Speaker - 6 Speaker
VA8 | Label - Spanish
VED | Decoration Pack-IV (Charcoal)
VEE | Bumper, FRT/RR - Body Color
VFT | B.I.W. Panel - Uncoated
VGC | Wrap Guard
VGP | Protector-Imp, Pedestrian
VH4 | Mud Guard
VIX | Visual V.I.N. Plate
VIY | Asterimark(*)
VK8 | Sunglasses Holder
VNR | VIN Model Year 2007
VNS | VIN Model Year 2008
VNT | VIN Model Year 2009
VNU | VIN Plate - US Type
VNW | VIN Plate - EURO Type
VOB | Radiator Grille - Chrome
VPQ | Wax Remover
W2V | Lettering - Trim Level - No Lettering
W6B | Seat Cover - Fabric - Woven, STD
W6G | Seat Cover - Fabric - Woven, DLX
WAL | Lettering - Car Name - Aveo
WCM | Lettering - Trim Level - "LT" Lettering
WU5 | Dimmer - Instrument Cluster
XA6 | ECE Label
XP7 | Lettering - Car Name - Barina
XXX | Audio System - Blank Cover, w/Deposit Box and Frame - DIN Size
XZ1 | Equipment - Hot Area
Y9Y | Badge - Chevrolet
Z5U | OSRVM, Turnover Type - Heating Function