For 1990-2009 cars

### Removal Procedure

1. Remove the EVAP canister vent solenoid valve.
2. Disconnect the inlet and outlet hose from the EVAP canister.
3. Remove the EVAP canister bracket retaining bolt.
4. Remove the EVAP canister (1).

### Installation Procedure

1. Install the EVAP canister (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the EVAP canister bracket retaining bolt and tighten to 8 N·m (71 lb in).
3. Connect the inlet and outlet hose to the EVAP canister.
4. Install the EVAP canister vent solenoid valve.