For 1990-2009 cars

#### Special Tools

J 28467-B (DW-117) Universal Engine Support Fixture

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Support the engine assembly using the J 28467-B .
3. Remove the engine mount bracket attaching bolts/nuts.
4. Remove the front timing belt cover. Refer to Timing Belt Cover Replacement.
5. Remove the engine mount attaching bolts/nuts.
6. Remove the engine mount.

### Installation Procedure

1. Install the engine mount.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the engine mount retaining bolts and tighten to 30 N·m (22 lb ft).
3. Install the front timing belt cover. Refer to Timing Belt Cover Replacement.
4. Install the engine mount bracket attaching bolts/nuts and tighten to 55 N·m (41 lb ft).
5. Remove the J 28467-B .
6. Connect the negative battery cable.