For 1990-2009 cars

### Removal Procedure

1. Remove the seat back. Refer to Front Seat Back Replacement.
2. Remove the seat cushion bolts.
3. Remove the cushion from the seat adjuster.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat cushion to the seat adjuster with the bolts and tighten to 25 N·m (18 lb ft).
2. Install the seat back. Refer to Front Seat Back Replacement.