For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
5th Gear Fork Bolts | 22 N·m | 16 lb ft
5th Gearshift Connector Bolts | 7 N·m | 62 lb in
Backup Lamp Switch | 20 N·m | 15 lb ft
Bearing Plate Bolts | 22 N·m | 16 lb ft
Bearing Retainer Bolts, Right Side | 25 N·m | 18 lb ft
Bearing-Adjusting Ring-Retainer Plate Bolt | 5 N·m | 44 lb in
Clutch-Release Cylinder Retaining Bolts | 20 N·m | 15 lb ft
Damping Block Connection Nut and Bolt | 80 N·m | 59 lb ft
Differential Cover Bolts | 40 N·m | 30 lb ft
Flywheel Inspection Cover Bolts | 7 N·m | 62 lb in
Gearshift Housing Bolts | 7 N·m | 62 lb in
Gearshift Lever Cover Bolts | 22 N·m | 16 lb ft
Input Driveshaft Detent Bolt | 15 N·m | 11 lb ft
Rear Damping Block Retaining Bolts | 55 N·m | 41 lb ft
Rear Mounting Bracket Bolts | 80 N·m | 59 lb ft
Ring-Gear Bolts | 70 N·m | 52 lb ft
Rod Clamp Bolt | 14 N·m | 124 lb in
Speedometer Housing Retaining Bolt | 4 N·m | 35 lb in
Speedometer-Driven Gear Bolt | 4 N·m | 35 lb in
Transaxle Cover Bolts | 18 N·m | 13 lb ft
Transaxle Lower Retaining Bolts (a) | 73 N·m | 54 lb ft
Transaxle Lower Retaining Bolt (b) | 31 N·m | 23 lb ft
Transaxle Lower Retaining Bolts (c) | 21 N·m | 15 lb ft
Transaxle Upper Retaining Bolts | 73 N·m | 54 lb ft
Transaxle Upper Mounting Bracket Bolts | 60 N·m | 44 lb ft