For 1990-2009 cars

## Inflatable Restraint Side Impact Sensor Replacement Except North America

### Removal Procedure

Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the trim from the center pillar.
3. Remove the side air bag sensor mounting bolts (1).
4. Remove the side air bag sensor (2).

### Installation Procedure

1. Install the side air bag sensor (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the side air bag sensor mounting bolts (1).

Tighten
Tighten the side air bag sensor mounting bolts to 10 N·m (89 lb in).

3. Install the trim to the center pillar.
4. Connect the negative battery cable.

## Inflatable Restraint Side Impact Sensor Replacement North America

### Removal Procedure

Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the trim from the center pillar.
3. Remove the side air bag sensor mounting bolts.
4. Remove the side air bag sensor.

### Installation Procedure

1. Install the side air bag sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the side air bag sensor mounting bolts.

Tighten
Tighten the side air bag sensor mounting bolts to 8 N·m (71 lb in).

3. Install the trim to the center pillar.
4. Connect the negative battery cable.